Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### BIOS Setup Utility Screens

The following table describes the functions of the seven top-level BIOS Setup screens.

Screen | Description
--- | ---
Main | General system information.
Advanced | Submenu level configuration information for the CPUs, IDE, SuperIO, HyperTransport, ACPI, Event Log, IPMI 2.0, MPS, PCI Express, Remote Access, USB, and Hardware Error Handling.
PCI/PnP | Plug-and-Play (PnP) devices can be configured by the BIOS (default) or by the operating system (if applicable).
Boot | Configure the boot device priority (hard disk drives and the ATAPI DVD-ROM drive).
Security | Install or change the user and supervisor passwords.
Chipset | Configuration options for the NorthBridge, SouthBridge, and PCI-X devices. Six separate screens can be accessed from the Chipset menu. Note that the Memory Chipkill option is enabled by default. Enabling Chipkill improves system reliability but might degrade system performance under some applications.
Exit | Save or discard changes.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |