Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

#### Bus Bar to DIMM Clearance Verification

To check the clearance between the DIMMs on a CPU module and the bus bars use a shim.

Legend
1 | Shim stock
2 | Bus bars
3 | Mylar covering

If the clearance is less than the minimum distance, a risk of damage to the DIMM modules exists when the CPU module is installed into its slot.

Legend
1 | CPU module with DIMMs
2 | Mylar cover on the bus bars
3 | Bus bars
4 | DIMM contacting the mylar on the bus bars

Return to Step 9 of the procedure, How to Install the Power Distribution Board.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |