Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Server Does Not Boot With Sun Multithreaded 10G Networking Card (6706575)

When using the default server BIOS settings, the server cannot boot when a Sun Multithreaded 10 Gigabit Networking Card (X1027A) is in PCIe slots 2, 3, or 4.

## Workaround

Disable the Multithreaded 10G Networking Card Option ROM from the server’s BIOS Setup utility. This preserves the option ROM space for the integrated RAID controller.

1. Enter the BIOS Setup utility by pressing the F2 key while the system is booting up and performing POST.
2. On the BIOS Main Menu screen, select the PCIPnP tab to open the PCI/PnP Settings screen.
3. Change the OpROM scanning field to “Disabled” for the slot in which the card is installed.
4. Save your changes and Exit the BIOS Setup utility.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |