Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install the Cover

1. Set the cover on the chassis so that the tabs on the cover align with the notches in the chassis.
2. Slide the cover toward the front of the server about 0.5 inches (12 mm.), ensuring that the front lip on the cover slides into the groove on the chassis.
3. Tighten the two captive screws on the back of the cover.

See Also

- How to Install the Front Bezel

- How to Prepare the Server for Operation

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |