Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Get the SP IP Address Using the BIOS Setup Utility

Before You Begin

- Complete the hardware setup as described in the hardware setup documentation.

- Apply standby power for your server by plugging an AC cord into the system power supply. See Server Connections for the location of the power cord connectors.

1. Reboot the server.
2. Press the F2 key when prompted, to access the BIOS Setup Utility.
3. In the BIOS Setup Utility, choose Advanced → IPMI 2.0 Configuration → Set LAN Configuration → IP address.

   The IP address for the SP is displayed.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |