Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

#### Accessing System Status Information Using the NMI Dump Swtich (SW3)

The Non-Maskable Interrupt (NMI) Dump switch (SW3 on the motherboard) sends an NMI order to the CPUs initiating a dump of system status information for debugging purposes. The NMI dump information is used for troubleshooting by service personnel and engineers. Do not press the NMI Dump switch unless instructed by service personnel.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |