Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove the Front Panel Indicator Board

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Remove all fan trays from the fan tray carriage. See How to Remove the Fan Tray.
3. Remove all CPU modules or CPU filler boards from the chassis. See How to Remove a CPU Module or Filler Card.
4. Remove the fan tray carriage from the chassis. See How to Remove the Fan Tray Carriage.
5. Disconnect the indicator board’s two flex cable connectors from the connectors on the front I/O board and the motherboard.

   Use the plastic-strip handles to gently pull the connectors straight up.

6. Remove the two screws securing the flex cable to the front panel and remove the flex cable.
7. Remove the two screws that secure the indicator board to the inside-front of the chassis.

See Also

- How to Install the Front Panel Indicator Board

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |