Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Compatible Racks

The slide rails are compatible with a wide range of equipment racks that meet the following standards:

- Four-post rack (mounting at both front and rear).

  Note - Two-post racks are not compatible.

- Rack should have horizontal opening and unit vertical pitch conforming to ANSI/EIA 310-D-1992 or IEC 60927 standards.

- Distance between front and rear mounting planes between approximately 26 to 34.5 inches (660.4 mm and 876.3 mm).

- Minimum clearance depth (to front cabinet door) in front of front rack mounting plane: 1 inch (25.4 mm).

- Minimum clearance depth (to rear cabinet door) behind front rack mounting plane: 31.5 inches (800 mm) with cable management arm (recommended) or 27.5 inches (700 mm) without the cable management arm.

- Minimum clearance width (between structural supports and cable troughs) between front and rear mounting planes: 18 inches (456 mm).

Note - The 4U Express Rail Rackmounting Kit card that is included with the slide rails and cable management assembly refers to the rack as a retma (Radio Electronics Television Manufacturers Association) rack.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |