Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Verify Slide-Rail Operation

Before You Begin

Perform the steps in How to Insert the Server Into the Rack.

1. To pull the server out of the rack, squeeze the front green lock levers and pull the server out of the rack until the slide rails reach their stops.
2. Push the server back into the rack until it reaches the internal stops.
3. To release the lock on the mounting brackets, locate the green plastic release tabs (on both left and right sides) on the mounting bracket.
4. With two hands, slide the green plastic tabs toward you to release the lock and push the server all the way into the rack.

Next Steps

Installing the Cable Management Arm (CMA)

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |