Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Configure the LSI BIOS

1. Set up your server so that you can respond to boot and POST messages. See Connecting to the System Console in Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server.
2. Power on or reboot the server.
3. Watch the display for the prompt that instructs you to press Ctrl-C to start the LSI configuration utility.

   `Press Ctrl-C to start LSI Logic Configuration Utility...`

4. When the prompt appears, press Ctrl-C.

   The LSI Configuration Utility main menu appears. For information about configuring RAID using LSI-based controllers that support integrated RAID, see the Sun LSI 106x RAID User's Guide (820–4933) at http://www.oracle.com/technetwork/indexes/documentation/index.html

See Also

- LSI BIOS Configuration Utility

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |