Skip Navigation Links
Exit Print View
| Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Get the SP IP Address By Using a Serial Connection and the CLI

Before You Begin

- Complete the hardware setup as described in the hardware setup documentation.

- Apply standby power for your server by plugging an AC cord into the system power supply. See Server Connections for the location of the power cord connectors.

1. Verify that your terminal, laptop, or terminal server is operational.
2. Configure the terminal device or the terminal emulation software running on a laptop or PC to the following settings:

   - 8N1: eight data bits, no parity, one stop bit

   - 9600 baud

   - Disable hardware flow control (CTS/RTS)

   - Disable software flow control (XON/XOFF)

3. Connect a serial cable from the RJ-45 SERIAL MGT port on the server’s back panel to a terminal device.

   See Server Connections for the location of the RJ-45 SERIAL MGT port.

4. Press Enter on the terminal device to establish a connection between that terminal device and the ILOM SP.

   The SP eventually displays a login prompt, such as the following example:

   `SUNSP` 0111AP0-0814YT06B4 `login:`

   In this example login prompt:

   - The string SUNSP is the same for all SPs.

   - 0111AP0-0814YT06B4is the product serial number by default. This value can also be the host name, which is assigned by the user or the DHCP server.

5. Log in to the ILOM.
   1. Type the default user name: `root`.
   2. Type the default password: `changeme`.

      Once you have successfully logged in, the SP displays its default command prompt:

      `->`

      You can now run CLI commands to configure ILOM for the server’s user accounts, network settings, access lists, alerts, and so on. For detailed instructions on CLI commands, see the Sun Integrated Lights-Out Manager 3.0 CLI Procedures Guide.

6. To display the SP IP address, type:

   `cd /SP/network`

   Note - You can switch back to the SP CLI from the serial console by entering the `Esc (` key sequence.

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |