Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install the Hard Disk Backplane

1. If necessary, perform the steps to remove the hard drive backplane. See How to Remove the Hard Disk Backplane.
2. Position the new hard drive backplane against the rear of the hard drive bay so that the holes in the backplane align with the screw holes in the chassis.
3. Replace and tighten the two screws that secure the hard drive backplane to the rear of the drive bays.

   Torque screws to 7 inch pounds (0.8 newton meters).

4. Tighten the single captive screw that secures the hard drive backplane.

   Torque screw to 7 inch-pounds (0.8 newton-meters).

5. Reconnect the flex cable connector to the rear of the hard drive backplane.
6. Reinstall all hard drives or hard drive fillers that you removed. See How to Install a Hard Drive.

   Note - Install the hard drives and hard drive fillers in the same slot from which you removed them.

7. Prepare the server for operation. See How to Prepare the Server for Operation.

See Also

- How to Remove the Hard Disk Backplane

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |