Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Power On All Server Components

This procedure powers on all server components and is different from applying standby power, which powers on the service processor only.

1. Verify that power cords have been connected and that standby power is on.

   In standby power mode, the Power/OK LED on the front panel blinks.

2. Use a pointed object to press and release the recessed Power button on the server front panel.

   When main power is applied to the full server, the Power/OK LED next to the Power button remains lit and no longer blinks.

   Figure Legend
   1 | Power/OK LED
   2 | Power button
   3 | USB connectors

Next Steps

To begin the initial SP configuration, see Communicating With the ILOM and the System Console

See Also

Controlling Power and Performing Hardware Reset in Sun Fire X4640 Server Service Manual

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |