Index

### Symbols

.properties command, 1

`/etc/aggregation.conf` file, 1

`/etc/hosts` file, 1

`/etc/modprobe.conf` file, 1

`/kernel/drv/nxge.conf` file, 1

### Numerics

1 GbE SFP Ethernet ports, 1

10 GbE SFP+ Ethernet ports, 1

10 GbE XAUI channels, 1

10 GbE XAUI PIN assignments, 1

10/100/1000 port, PIN location, 1

10/100/1000BASE-T, 1

10-Gigabit Ethernet ports, 1

10-Gigabit XAUI interface, 1

3-PIN per column, 1

### A

ACT, LED, 1

aggregation, 1

`aggrkey`, 1

airflow conditions, 1

AMC Module Management Controllers, 1

AMC modules

installation, 1

supporting hot-swap, 1

antistatic wrist strap, 1

applications, terminating, 1

ARTM, shut down, 1

ATCA shelf (chassis), 1

auto negotiate, 1

### B

back-to-back slots, 1

barcode labels, 1

blade servers, supported, 1

BLUE LED, 1, 2, 3

Board Info Area, 1

board removal, 1

`bond0` interface, 1

bonding driver, 1

boot process, 1

### C

certifications, 1

`checksum`, 1

classification variables, 1

`clia` command, 1

commands, IPMI, 1

compatible node boards, 1

compliance, EMI, 1

`configtool` utility, 1

connector mates, 1

connector PIN outs, 1

connectors and PIN assignments, 1

CPU

load balancing, 1

thread affinity, 1

CRC32C support, 1

### D

data corruption, 1

depth, 1

device instance, specifying, 1

digital components, 1

direct pass-through connections, 1

disabled ports, 1

`dladm` command line utility, 1

`dladm` `show`-`aggr` `-L`, displaying LACP, 1

`dladm` `show`-`aggr -s` command, displaying statistics, 1

`dladm`(1M) man page, 1

DMA channels, 1, 2

DMAs, 1

driver

bonding, 1

`nxge`, 1

parameters, listing, 1

statistics, 1

duplex LC fiber connector, 1

### E

e-Keying port assignments, 1

electromagnetic emissions, 1

electromagnetic interference (EMI, 1

electronic keying (e-Keying), 1, 2

electrostatic discharge (ESD), 1

electrostatic discharge effects, 1

EMI, electromagnetic interference, 1

empty chassis, installing boards, 1

energy hazards, 1

environmental specifications, 1

ESD precautions, 1

Ethernet

`ethtool` utility, `-S` option, 1

interfaces, configuring, 1

interfaces, configuring Jumbo Frames, 1

management port, 1

packet traffic, 1

ports, tuning, 1

tag header format, 1

### F

fail-safe flash update, 1

`fcode` firmware, 1

file corruption, 1

firmware, 1

first mate, 1

flow classification, 1

flow template, 1

front- and rear-board installations, 1

front ATCA node board, 1

FRU data records, 1

FRU information, 1

FRU Information Storage Definition, 1

full duplex ports, 1

functional interconnect, 1

### G

Gigabit Ethernet driver, 1

GREEN LED, 1

### H

header parsing, 1

height board, 1

host board

compatible, 1

PCI-express communication, 1

slot, 1

host chassis, selection criteria, 1

host names, 1

guidelines, 1

`hostname.nxge` file, 1

hotswap communication, 1

hot-swap insertion, 1

hot-swap software, 1

HS, LED, 1

### I

I/O interfaces, 1

I2C

connection, 1

hang recovery, 1

serial bus, 1

ID 15, 1

IEEE 1101.11 mechanical standards, 1

IEEE 802.3 Ethernet standard, 1

IEEE 802.3 MAC clients, 1

IEEE 802.3ad, 1

`ifconfig` utility, 1

Inlet air temperature, 1

installing, 1, 2

instance numbers, 1

Intelligent Platform Management Interface (IPMI), 1

IP address, 1

IP class, 1

IPMB-L

address, 1

bus, 1

IPMI commands, 1

### J

J32/P32 Zone-3 connector, 1

Jumbo Frames

commands, 1

configuring, 1

support, 1

### K

`kstat` command, 1

### L

L1 to L4 IPv4/v6 header parsing, 1

last mate, 1

Layer 2 configuration. viewing, 1

Layer 3 configuration, viewing, 1

layer configuration, 1

LC connectors, 1

LEDs

ACT, 1

AMBER, 1

back panel, 1

BLUE, 1, 2, 3

Ethernet management port, 1

GREEN, 1, 2

HS, 1

LNK, 1

OK, 1

OOS, 1, 2

software control, 1

link aggregation, 1

configuring in a Linux environment, 1

configuring in a Solaris environment, 1

group, 1

status, 1

LNK, LED, 1

### M

MAC addresses, 1

MAC clients, 1

mates, 1

maximum link speed, 1

maximum transmission unit (MTU), configuration, 1

midplane, 1

modprobe nxge, 1

Module Management Controller (MMC), 1, 2

### N

`ndd` utility, 1

NEBS certifications, 1

network devices

listing on Linux host, 1

listing on SPARC host, 1

network interface, configuring, 1

networking I/O virtualization, 1

node boards, compatible, 1

`nxge` driver, 1

configuration file, 1

configuring, 1

installing on Linux OS systems, 1

installing on Solaris OS systems, 1

interfaces, 1

removing, 1

`nxge` instance numbers, preserving, 1

`nxge` interfaces, 1

`nxge.conf` file, 1

### O

OK, LED, 1

OOS

LED, 1

LEDs, 1

OpenBoot (ok) prompt, 1

operating systems, 1

optical transceiver, 1

### P

P30, power PIN assignment, 1

P32, management infrastructure PIN assignments, 1

P33, management infrastructure PIN assignments, 1

packet counts, 1

packets

distributed, 1

sending and receiving large, 1

size, 1

packing list, 1

packing material, 1

parallelism, extending, 1

parameters

configuring driver on Linux, 1

configuring driver on Solaris OS, 1

listing for Linux, 1

listing for Solaris OS, 1

modifying in `nxge.conf` file, 1

modifying with `ndd` utility, 1

persistence, 1

RX coalesce, 1

part number, 1

pass-through, 1

PCI devices

listing on Solaris OS, 1

listing on x86 host, 1

PCI Industrial Computer Manufacturers Group (PICMG) specifications, 1

PCI-express signals, enabling, 1

performance, tuning ports on Linux, 1

persistence, 1

physical dimensions, 1

physical point of attachment (PPA), 1

PICMG AMC.0 specification, 1

PIN header assignment, 1

PINs

10/100/1000 Mb management port, 1

assignments, 1

bent or damaged, 1

common, 1

details, 1

port commands, compliance, 1

ports, 1

1 GbE SFP Ethernet, 1

10 GbE Ethernet, 1

10-Gigabit Ethernet, 1

auto negotiate, 1

disabled, 1

e-Keying assignments, 1

Ethernet management, 1

features, 1

full duplex, 1

MAC addresses, 1

RS232 serial console, 1

serial console management, 1

SFP, 1

tuning on Linux, 1

power requirements, 1, 2

powering down, 1

pressure drop, 1

### R

rails, alignment, 1

RDC groups, 1

reboot, 1

redirect traffic, 1

removing, 1, 2

RJ-45 connector, 1

RJ-45 connector jack, 1

RJ45 management ports, 1

RS232 serial console port, 1

RS232 signaling, 1

RX and TX packets, 1

RX coalesce parameters, 1

RX, signal receiver, 1

### S

`-S` option, `ethtool`, 1

second mate, 1

sensor data records (SDRs), 1

serial console management port, 1

serial number, 1

SFP

connections, 1

modules, 1

ports, 1

shelf manager, 1

shut down, 1

signals, 1

receiver, 1

source, 1

single mode or multimode, 1

slot filler panel, 1

slot usage, 1

slot, compatible host, 1

small form-factor pluggable (SFP), 1

Solaris 10 (SPARC) Operating System, 1

Solaris 10 (x86) Operating System, 1

specifications, 1

statistics, driver, 1

Sun MAC controller, 1

### T

terminating applications, 1

thermal simulation model, 1

TX, signal source, 1

### U

UL60950-1, compliance, 1

unpacking, 1

updates, firmware, 1

upgrading instructions, 1

utility

`configtool`, 1

`ifconfig`, 1

`ndd`, 1

### V

verifying installation, 1

virtualization, 1

VLANs

configuration parameters, 1

configuring, 1

configuring in a Linux environment, 1

configuring in Solaris environment, 1

defining, 1

ID (VID), 1

tagged format, 1

virtual device, 1

Voltage monitoring, 1

voltages, 1

### W

Wind-River Linux 4.0, 1

### X

x8 PCIe, 1

### Z

Zone 3 connector complex, 1

Zone 3 connectors, 1

Copyright © 2008 Sun Microsystems, Inc. All Rights Reserved.