Exit Print View
#### Sun Netra X6270 M2 Server Module Installation Guide for Windows Operating Systems |

| Part I Windows Server Installations |

Chapter 4

## Post Installation of Windows Server 2008

After completing the installation of the Windows Server 2008 (SP2 or R2) operating system and rebooting the server module, you should review the following post installation tasks and, if necessary, perform the tasks that are applicable to your server module.

- Installing Critical Device Drivers and Supplemental Software

- Installing Supplemental Software

- Configuring Support for TPM

- Configuring Intel NIC Teaming

### Before You Begin

The procedures in this chapter assume that you have:

- Installed the Microsoft Windows Server operating system

- Obtained a copy of the Tools and Drivers DVD.

  If you do not have a copy of the Tools and Drivers DVD, you can download the latest ISO image of the Tools and Drivers DVD from the product download site. For Instructions see, Appendix D, Downloading the ISO Image for the Tools and Drivers DVD.

### Installing Critical Device Drivers and Supplemental Software

An installation wizard is provided on the Tools and Drivers DVD to install server module-specific device drivers and Supplemental Software. The server module-specific device drivers are provided to support optional hardware devices that can be installed on your server module.

# Install Server Module-Specific Device Drivers

1. Insert the Tools and Drivers DVD into a local or remote USB DVD drive and do one of the following:
   - If the DVD automatically starts, click `Install Drivers and Supplement Software`.
   - If the DVD does not automatically start, navigate to one of the following folders containing the appropriate `InstallPack` file (for example, `InstallPack_1_0_1.exe`), and double-click it.
     - <DVD>/Windows/W2K8/Packages
     - <DVD>/Windows/W2K8R2/Packages

       The Server Installation Package dialog appears.

2. In the Install Pack dialog, click `Next` to accept the default installable items.

   Note - You should always accept the “default installable items” to ensure that the most recent versions of the drivers are installed.

   The Install Pack notice dialog appears.

3. In the Install Pack notice dialog, read the message, then click `Next`.

   The Welcome to the Sun Fire Installation Wizard appears.

4. In the Welcome to the Sun Fire Installation Wizard dialog, click `Next`.

   The End User License Agreement page appears.

5. In the End User License Agreement page, select `I Accept This Agreement`, then click `Next`.

   The platform-specific drivers are installed. A green check mark verifies that each driver was installed successfully.

6. In the Driver Installation Pack dialog, click `Finish`.

   The System Settings Change dialog appears.

   Note - If you plan on installing Supplemental Software (highly recommended), do not restart your system at this time. Once the Supplemental Software has been installed, you will be prompted to restart the system.

7. Perform one of the following:
   - If you accepted the default installable settings in Step 2, click `No` to proceed to Installing Supplemental Software.
   - If you are not installing the Supplemental Software, click `Yes` to restart your computer.

### Installing Supplemental Software

There are several Supplemental Software components available for your server module. You have two options for installation:

- Typical: Installs all Supplemental Software applicable for your server module.

- Custom: Installs only the Supplement Software selected for installation.

Install Pack Optional Supplemental Software identifies the optional Supplemental Software components available for your server module.

###### Install Pack Optional Supplemental Software

Available Supplemental Software Components | Server modules With LSI Integrated RAID Controller | Server modules With Intel Integrated Disk Controller
--- | --- | ---
LSI MEGARAID Storage Manager, click `Yes` to restart your computer Enables you to configure, monitor, and maintain RAID on the SAS internal RAID host bus adapter (HBA). | Typical | Not applicable
IPMItool command-line utility The IMPItool command-line utility reads the sensor data repository (SDR) and displays sensor values, system event log (SEL), and field- replaceable unit (FRU) inventory information; gets and sets LAN configuration parameters; and performs chassis power control operations via the BMC (also called the service processor (SP). | Typical | Typical
Intel NIC Teaming Enables the network interfaces on a server module to be grouped together into a team of physical ports called a virtual interface. | Typical | Typical

# Install the Supplemental Software

| Caution - If you have already installed the Supplemental Software, running the installation again will not necessarily reinstall the Supplemental Software. It might result in the components being removed. Carefully review the dialog boxes during Supplemental Software installation to ensure that the results are as expected.

1. Do one of the following:
   - If you did not select the Supplemental Software when you ran the procedure Installing Critical Device Drivers and Supplemental Software, refer back to that procedure and run it again, but this time accept the default settings in Step 2 (the default is to install the Supplemental Software), and select No in Step 7.
   - If you did select Supplemental Software at the Server Installation Package dialog box in Step 2 of Installing Critical Device Drivers and Supplemental Software, and selected No in Step 7, the Install Pack Supplemental Software dialog appears. Proceed to Step 2.
2. In the Install Pack Supplement Software dialog, click `Next` to accept the typical settings; or select `Custom` to choose the options to install (see descriptions of the Supplemental Software in Install Pack Optional Supplemental Software ).

   The Component Installation wizard will guide you through the installation of each of the selected Supplemental Software components.

3. After the Supplemental Software has been installed, click `Finish`.
4. Click `Yes` at the System Setting Change dialog to restart your system.

   If you ran the Sun Server Installation Package software from the Tools and Drivers DVD, remove the DVD from your system.

### Configuring Support for TPM

If you intend to use the Trusted Platform Module (TPM) feature set that is provided in Windows 2008, you must configure the server module to support this feature. For instructions, see the configuring support for TPM information in the Sun Netra X6270 M2 Server Module Service Manual, 821-0939.

Note - TPM enables you to administer the TPM security hardware in your server module. For additional information about implementing this feature, refer to the Windows Trusted Platform Module Management documentation provided by Microsoft.

### Configuring Intel NIC Teaming

For more information on setting up NIC teaming for your environment, refer to the Intel Connectivity web page on Advanced Networking Services Teaming at:

http://support.intel.com/support/network/sb/CS-009747.htm

Additionally, you can download the complete set of Intel Network Connections User Guides for your server module’s network adapters at:

http://support.intel.com/support/network/sb/cs-009715.htm

Copyright © 2010 , Oracle and/or its affiliates. All rights reserved. Legal Notices |