A P P E N D I X A

Server Module Specifications

This appendix contains physical specifications for the server module. Refer to the chassis documentation for additional server module specifications.

- Physical Specifications

- Electrical Specifications

- Environmental Requirements

##

A.1 Physical Specifications

The Sun Netra X6270 M2 server module is designed to be installed in a Sun Netra 6000 DC modular system.

TABLE A-1 gives the physical specifications for the server module.

TABLE A-1 Physical Specifications
| English | Metric
--- | --- | ---
Height | 12.87 inches | 327 mm
Width | 1.7 inches | 44 mm
Depth | 20.16 inches | 512 mm
Weight | 17 pounds | 7.71 kg

##

A.2 Electrical Specifications

The server moduel is 12.9 x 20.1 x 1.7 inches. The server module connects to Sun Netra 6000 DC modular system, or chassis, which provides 12V main power to each module, as well as cooling through fans. In addition to the 12V main power, the chassis provides 3.3V AUX power to each server module to power the local FRU ID EEPROM. This 3.3V AUX power enables the chassis monitoring module (CMM) to query each server module slot prior to 12V main power and 12V fan power application to validate that there is sufficient power and cooling to support the server modules installed in the chassis.

##

A.3 Environmental Requirements

TABLE A-2 gives the environmental requirements for the server module.

TABLE A-2 Environmental Requirements
Condition | Requirement
--- | ---
Operating temperature | 5 oC to 35 oC noncondensing
Nonoperating temperature | -40 oC to 65 oC
Operating humidity | 10% to 90% noncondensing (27 oC max. wet bulb)
Nonoperating humidity | 93% noncondensing (38 oC max. wet bulb)
Operating altitude | 3048 meters at 35 oC
Nonoperating altitude | 12,000 meters

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.