Exit Print View
#### Sun Netra X6720 M2 Server Module Installation Guide for Linux, Virtual Machine Software, and Oracle Solaris Operating Systems |

| Part II Virtual Machine Software Installations |

Chapter 8

## Installing VMware ESX or ESXi

This chapter summarizes the necessary steps for installing:

- VMware ESX 4.0 Update 1 (and subsequent releases)

- VMware ESXi 4.0. Update 1 (and subsequent releases)

This chapter includes the following topics:

- Installing VMware ESX or ESXi Using Local or Remote Media

- VMware ESX and ESXi Post Installation Tasks

### Installing VMware ESX or ESXi Using Local or Remote Media

The procedures in this section describe how to install the VMware (ESX or ESXi) software from local or remote media. It assumes that you are booting the VMware installation media from one of the following sources:

- VMware ESX or ESXi 4.0 Update 1 CD or DVD (internal or external CD or DVD)

- VMware ESX or ESXi 4.0 Update 1 ISO image (network repository)

Note - The VMware ISO image can be used for remote installations or for creating an installation CD or DVD.

Refer to the following procedures to install the VMware software from local or remote media:

- Install VMware ESXi 4.0 From Local or Remote Media

- Install VMware ESX 4.0 From Local or Remote Media

#### Before You Begin

Prior to performing the installation, the following requirements must be met:

- All applicable installation considerations for installing the virtual machine software should have been met. For details, see VM Software Installation Considerations.

- Gather the VMware ESX or ESXi documentation. This documentation should be used in conjunction with the installation procedure presented in this chapter.

  The VMware ESX and ESXi documentation is available at:

  http://www.vmware.com/support/pubs/vs_pubs.html

- For VMware ESX installations, determine the network management interface you will use for the VM service console.

  The VM service console and management interface require a network interface. The service console does not automatically use the first interface with a live connection. Therefore, you will need to select a network interface for the service console during installation since the network interface defaults to vmic0.

# Install VMware ESXi 4.0 From Local or Remote Media

1. Ensure that the install media is available to boot.
   - For CD/DVD distribution media. Insert the VMware ESXi 4.0 Update 1 Distribution media boot disc (CD labeled number 1 or the single DVD) into the local or remote USB CD/DVD-ROM drive.
   - For ISO images. Ensure that the ISO images are available and that the boot disc image (CD labeled number 1 or DVD) has been selected in the ILOM Remote Console application (`Devices menu`-->`CD-ROM Image`).

   For additional information about how to set up the installation media, see Appendix A, Supported Installation Methods.

2. Reset the power on the server.

   For example:

   - From the ILOM web interface, select the `Remote Control` --> `Remote Power Control`, then select `Reset` from the `Select Action` list box.
   - From the local server, press the Power button (approximately 1 second) on the front panel of the server to power off the server, then press the Power button again to power on the server.
   - From the ILOM CLI on the server SP, type: `reset /SYS`
   - From the ILOM CLI on a CMM, type: `reset /CH/BLn/SYS`

     Where n is the number of server module in chassis.

   The BIOS screen appears.

   Note - The next events occur very quickly; therefore, focused attention is needed for the following steps. Watch carefully for these messages as they appear on the screen for a brief time. You might want to enlarge the size of your screen to eliminate scroll bars.

3. In the BIOS power-on self-test screen, press F8 to specify a temporary boot device for the VMware installation.

   The Please Select Boot Device menu appears.

4. In the Boot Device menu, select either the external or virtual CD/DVD device as the first boot device, then press Enter.

   The device strings listed in the Boot Device menu are in the following format: device type, slot indicator, and product ID string.

   After a few seconds, the splash screen for the VMware installation program appears.

5. To complete the installation, refer to the VMware ESXi 4.0 Update 1 installation documentation.

   You can access the VMware ESXi 4.0 installation documentation at: http://www.vmware.com/support/pubs/vs_pubs.html

6. After installing VMware ESXi 4.0 Update 1, proceed to VMware ESX and ESXi Post Installation Tasks.

# Install VMware ESX 4.0 From Local or Remote Media

1. Ensure that the install media is available to boot.
   - For Distribution CD/DVD. Insert the VMware ESX 4.0 Update 1 Distribution media boot disc (CD labeled number 1 or the single DVD) into the local or remote USB CD/DVD-ROM drive.
   - For ISO images. Ensure that the ISO images are available and that the boot disc image (CD labeled number 1 or DVD) has been selected in the ILOM Remote Console application (`Devices` menu-->`CD-ROM Image`).

   For additional information about how to set up the installation media, see Appendix A, Supported Installation Methods.

2. Reset the power on the server.

   For example:

   - From the ILOM web interface, select `Remote Control` --> `Remote Power Control`, then select the `Reset` option from the `Select Action` list box.
   - From the local server, press the Power button (approximately 1 second) on the front panel of the server to power off the server, then press the Power button again to power on the server.

     Note - The next events occur very quickly; therefore, focused attention is needed for the following steps. Watch carefully for these messages as they appear on the screen for a brief time. You might want to enlarge the size of your screen to eliminate scroll bars.

3. In the BIOS power-on self-test screen, press F8 to specify a temporary boot device for the VMware installation.

   The Please Select Boot Device menu appears.

4. In the Boot Device menu, select either the external or virtual CD/DVD device as the first boot device, then press Enter.

   The device strings listed in the Boot Device menu are in the following format: device type, slot indicator, and product ID string.

   After a few seconds, the splash screen for the VMware installation program appears.

5. Continue the VMware installation program and, when necessary, refer to the VMware ESX 4.0 installation documentation.
6. When the Network Configuration dialog appears, perform the following steps:
   1. In the Network Adapter field, click the drop-down arrow and select the desired network adapter, then click `Next`.

      In this dialog, a live network adapter (that is, an adapter connected to the network) must be specified for the VMware service console (`vmnic0`). Each network adapter that is live has a green check mark next to it as shown in the above dialog. Also, notice that the MAC address that is associated with the network port (for example: `NET0`, `NET1`, `NET2`, or `NET3`) appears. You can use the MAC address to determine which physical network port is present.

      Alternatively using the ILOM command-line interface (CLI), you can determine the MAC addresses that are associated with the server’s physical network ports. For example, in the ILOM CLI you would type the following command to determine the MAC address that is associated with the physical network port known as `NET0`:

      `->` `show /SYS/MB/NET0`

      In the sample output shown below, the MAC address for NET0 is 00:14:4F:CA:B8:36.

          ->show /SYS/MB/NET0
           /SYS/MB/NET0
           Targets:
           Properties:    type = Network Interface
           ipmi_name = MB/NET0
           fru_name = GIGABIT ETHERNET CONTROLLERS
           fru_manufacturer = INTEL
           fru_part_number = 82575EB
           fru_serial_number = 00:14:4F:CA:B8:36
           fault_state = OK
           clear_fault_action = (none)

      Note - If you are unsure which network adapter to select, contact your network administrator.

      The ESX 4.0 Network Configuration dialog appears enabling you to specify the network adapter settings.

   2. In the Network Configuration dialog, do one of the following:
      - To auto-configure the network adapter, select `Set automatically using DHCP`, then click `Next`.

        - or -

      - To manually configure the network adapter, select `Use the following network settings`, and specify the network settings in the appropriate fields, then click `Next`.
7. Complete the VMware ESX 4.0 Server installation and, when necessary, refer to the VMware ESX 4.0 Server installation documentation.
8. After completing the installation, proceed to VMware ESX and ESXi Post Installation Tasks.

### VMware ESX and ESXi Post Installation Tasks

After completing the ESX or ESXi installation, review the following post installation tasks and, if necessary, perform the tasks that are applicable to your system.

- Configure Network Adapters for VMware ESXi Installations

- Local Storage Drive Not Seen After Performing VMware ESXi Installation

- Update the ESX or ESXi Operating System

- Manage VMware Resources

#### Configure Network Adapters for VMware ESXi Installations

The following procedure describes how to configure the VMware ESXi settings for the network adapter(s) installed on your server. These instructions also include steps for discovering the physical port location of each network adapter installed on your server.

# Configure Network Adapter Settings

1. Log in to the VMware ESXi Server.
2. Access the System Customization dialog and select `Configure Management Network`.

   The Configure Management Network dialog appears.

3. In the Configuration Management Network dialog, select `Network Adapters`.

   The Network Adapters dialog appears.

4. In Network Adapters dialog, select a live network adapter (that is, an adapter connected to the network) for the VMware service console (`vmnic0`), then press Enter.

   A live network adapter (that is, an adapter connected to the network) must be specified for the VMware service console (vmnic0). Notice that the MAC address that is associated with the server’s physical network port (for example: `NET0`, `NET1`, `NET2`, or `NET3`) is displayed in the Hardware Label column. Therefore, you can use the MAC address to determine which of the server’s physical network ports are being displayed. For example, to determine the MAC address for each server network port, enter the following command in the ILOM command-line interface (CLI) for each server network port:

   -> `show` `/SYS/MB/NET` n

   Where is n is 0, 1, 2, or 3

   If the network adapter shown in the above dialog were associated for network port `NET0`, then the CLI command `show /SYS/MB/NET0`, would produce the following output, where the `fru_serial_number` field lists the MAC address.

       -> show /SYS/MB/NET0
        /SYS/MB/NET0
        Targets:
        Properties:
        type = Network Interface ipmi_name = MB/NET0
        fru_name = GIGABIT ETHERNET CONTROLLERS
        fru_manufacturer = INTEL
        fru_part_number = 82576EB
        fru_serial_number = 00:21:28:3D:B7:96
        fru_extra_2 = 00:21:28:3D:B7:96
        fault_state = OK
        clear_fault_action = (none)

   Note - If you are unsure of which network adapter to select, contact your network administrator.

#### Local Storage Drive Not Seen After Performing VMware ESXi Installation

If your local storage drive on the server is attached to a Sun Storage 6 Gb SAS Host Bus Adapter (SG-SAS6-EM-Z, SG-SAS6-REM-Z, or SGX-SAS6-REM-Z), the VMFS datastore on the local storage drive is not visible after performing the VMware ESXi installation. In this case, perform the following procedure to make the existing VMFS datastore on the local storage drive visible and ready for use.

# Make Local VMFS Datastore Visible to VSphere Client

1. Connect to the VMware ESX server by using the VSphere Client.
2. In the VSphere Client interface add the ESXi host to the datacenter of your choice.
3. Select the ESXi host that you added to the datacenter in Step 2, then click the `Configuration` tab.
4. In the Configuration tab, do the following:
   1. In the Hardware box, select `Storage,` then click the `Add Storage` link.
   2. Verify that the `Disk/LUN Storage Type` is selected, then click `Next`.
   3. Select the `vmhba` entry that corresponds to the local disk, then click `Next`.
   4. Select `Use Free Space`, then click `Next`.
   5. Create a datastore name (for example, `local_storage`), then click `Next`.
   6. Adjust the maximum file size if needed, then click `Next`.
   7. Verify that the proposed disk layout is acceptable, then click `Finish`.

      The local VMFS datastore is visible and ready for use.

#### Update the ESX or ESXi Operating System

The VMware ESX or ESXi installation media might not contain the most up-to-date versions of the software.

If necessary, update the ESX or ESXi Server software with the latest updates and patches. For download instructions, see this web site:

http://support.vmware.com/selfsupport/download/

It is recommended to install patch ESX400-201002001 for ESX or patch ESXi400-201002001 for ESXi.

#### Manage VMware Resources

To learn more about configuring and managing VMware resources, refer to the VMware documentation at:

http://www.vmware.com/support/pubs/vs_pages/vsp_pubs_esxi40_i_vc40.html

Copyright © 2010 , Oracle and/or its affiliates. All rights reserved. Legal Notices |