A P P E N D I X C

Connector Pinouts

This appendix contains information about the following connector pinouts:

- 3-Cable Dongle Pinouts

- SAS/SATA Connectors

- SAS Diskplane

- SAS Power/LED Connector

##

C.1 3-Cable Dongle Pinouts

The following figure and table provides pinout information for the 3-cable dongle connectors.

FIGURE C-1 3-Cable Dongle Connectors (P/N 530-3936 Option # 4622A)

Figure Legend Pinouts for 3-Cable Dongle Connectors (Option# 4622A)
3 RJ-45 | RJ-45 Serial Signal | 2 USB | USB Signal | 1 VGA | VGA Signal
--- | --- | --- | --- | --- | ---
1 | RTS | 1 | USB1 VCC | 1 | Red
2 | DTR | 2 | USB1 DN | 2 | Green
3 | Trasnmit Data | 3 | USB1 DP | 3 | Blue
4 | Ground | 4 | USB1 Ground | 4 | Not used
5 | Ground | 5 | USB2 Ground | 5 | Ground
6 | Recive Data | 6 | USB2 DP | 6 | Ground
7 | DSR and DCD | 7 | USB2 DP | 7 | Ground
8 | CTS | 8 | USB2 Ground | 8 | Ground
9 | 5V
10 | Ground
11 | Ground
12 | VGA Data
13 | H_Sync
14 | V_Sync

##

C.2 SAS/SATA Connectors

The Serial Attached SCSI (SAS)/Serial Advanced Technology Attachment (SATA) connector pins and their corresponding descriptions are shown in the figure and table in this section.

FIGURE C-2 SAS/SATA Connector

TABLE C-1 SAS/SATA Connector Pins
Segment | Pin Number | Pin Name | Description
--- | --- | --- | ---
Signal Segment | S1 | Gnd | Second mate ground
S2 | TX+ | Positive side of transmit to hard drive
S3 | TX- | Negative side of transmit to hard drive
S4 | Gnd | Second mate ground
S5 | RX- | Negative side of receive from hard drive
S6 | RX+ | Positive side of receive from hard drive
S7 | Gnd | Second mate ground
Backside Signal Segment | S8 | Gnd | Second mate ground
S9 |  | Not used
S10 |  | Not used
S11 | Gnd | Second mate ground
S12 |  | Not used
S13 |  | Not used
S14 | Gnd | Second mate ground
Power Segment | P1 | 3.3 V | Not used
P2 | 3.3 V | Not used
P3 | 3.3 V | Not used
P4 | Gnd | First mate ground
P5 | Gnd | Second mate ground
P6 | Gnd | Second mate ground
P7 | 5.0 V | Pre-charge, second mate
P8 | 5.0 V |
P9 | 5.0 V |
P10 | Gnd | Second mate ground
P11 | Ready LED | Activity/Ready LED
P12 | Gnd | First mate ground
P13 | 12.0 V | Pre-charge, second mate
P14 | 12.0 V |
P15 | 12.0 V |

##

C.3 SAS Diskplane

The SAS diskplane connector pins and their corresponding descriptions are listed in the following table.

TABLE C-2 SAS Disk Backplane Signal Connector Pins
Pin Number | Signal Name
--- | ---
1, 4, 7 | GND
2, 3 | TX+/TX-
5, 6 | RX+/RX-

##

C.4 SAS Power/LED Connector

The SAS power/LED connector pins and their corresponding descriptions are shown in the figure and table in this section.

FIGURE C-3 SAS Power/LED Connector

TABLE C-3 SAS Power/LED Connector Pins
Pin Number | Signal Name
--- | ---
1 | DISK1_FAULT_LED_L
2 | DISK1_RDY2RM_L
3 | DISK1_PRSNT_L
4 | 12V
5 | GND
6 | DISK0_FAULT_LED_L
7 | DISK0_RDY2RM_L
8 | DISK0_PRSNT_L
9 | GND
10 | 5V

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.