Sun Java System Application Server Enterprise Edition 8.1 2005Q2 Deployment Planning Guide

- Previous: Choosing Network Cards
- Next: Planning for Availability

## Network Settings for HADB

Note –

HADB uses UDP multicast and thus you must enable multicast on your system’s routers and host network interface cards. If HADB spans multiple sub-networks, you must also enable multicast on the routers between the sub-networks. For best results, put HADB nodes all on same network. Application server instances may be on a different sub network.

The following suggestions will enable HADB to work optimally in the network:

- Use switched routers so that each network interface has a dedicated 100 Mbps or better Ethernet channel.

- When running HADB on a multi-CPU machine hosting four or more HADB nodes, use 1 Gbps Ethernet cards. If the average session size is greater than 50 KB, use 1 Gbps Ethernet cards even if there are less than four HADB nodes per machine.

- If you suspect network bottlenecks within HADB nodes:

  - Run network monitoring software on your HADB servers to diagnose the problem.

  - Consider replacing any 100 Mbps Ethernet cards in the network with 1 Gbps Ethernet cards.

- Previous: Choosing Network Cards
- Next: Planning for Availability

- © 2010, Oracle Corporation and/or its affiliates