Go to main content
oracle home

# Sun Fire X4470 Server Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: September 2018

- Sun Fire X4470 Server Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Sun Fire X4470 Product Notes

- Server Security, Software Releases, and Critical Patch Updates

- IMPORTANT - Install Latest OS Updates, Patches, and Firmware

- Changes to TLSv1.1 Configuration Property as of ILOM 4.0.3.x
- Oracle ILOM File Transfer Using URI Fails if Target Password Contains Special Characters (25917655)
- Diagnosing SAS Data Path Failures on Servers Using MegaRAID Disk Controllers
- Deprecation Notice for Oracle ILOM IPMI 2.0 Management Service
- Resolving Warning Messages for Custom CA and Self-Signed SSL Certificates
- Oracle ILOM License Information
- Supported Operating Systems
- Supported Operating Systems
- Supported Operating Systems in Software Releases
- Available Preinstalled Operating Systems
- Oracle Unbreakable Enterprise Kernel for Linux
- Supported Firmware and Software
- Supported Firmware in Software Releases
- Firmware Updates
- Supported Software
- Downloading an OS or Software Applications
- Supported PCIe Cards
- Quantity and Slot Restrictions
- Minimum Firmware Revisions for PCIe Cards
- Sun Flash Accelerator F20 PCIe Card Requirements
- Card Placement and Cooling
- ESM Replacement Interval
- Internal Sun Storage 6Gb SAS PCIe RAID HBA Requirements
- Sun Storage 10GbE FCoE PCIe Low Profile Dual Port CNA and OS Support
- Oracle x86 Products Accessibility

- Hardware Accessibility
- Oracle ILOM Accessibility
- Oracle Hardware Management Pack Accessibility
- BIOS Accessibility
- Documentation Accessibility

- Known Open Issues
- Hardware Known Issues
- Firmware Known Issues
- BIOS Known Issues
- Oracle ILOM Known Issues
- Oracle Solaris Known Issues
- Oracle Linux, SUSE Linux Enterprise Server (SLES), Red Hat Enterprise Linux (RHEL), and Oracle VM Known Issues
- Windows Known Issues
- Documentation Known Issues
- Broken Links in Sun Server X4470 Documentation Library
- Getting Firmware and Software Updates

- Firmware and Software Updates
- Options for Accessing Firmware and Software Updates
- Software Releases
- Getting Updates From Oracle Hardware Installation Assistant or My Oracle Support
- Download Firmware and Software Updates From My Oracle Support
- Installing Updates Using Other Methods
- Oracle Support

Language:

### Hardware Known Issues

Table 5 Hardware Known Open Issues
Bug ID | Description
--- | ---
15629239 | SMI Link Spare Lane Is Reported as Faulty Issue: The Scalable Memory Interconnect (SMI) link that connects the processor to a memory buffer includes a spare lane in each direction to provide redundancy in the event that one of the other lanes in the link fails. This spare lane will not be used unless one of the other lanes in the link fails. Under certain rare circumstances this spare lane is reported as faulty when booting the system. Oracle ILOM will detect this error and diagnose a fault.memory.intel.branch.spare-lane-failover fault that is attributed to the memory riser to which the lane is routed. The spare lane is provided only for redundancy and there is no impact to normal system operation if the link does not experience an additional lane failure. There is no performance impact associated with this error. Affected Hardware: Sun Fire X4470 Server Workaround: Clear the riser fault and power cycle the system using the following Oracle ILOM command-line interface (CLI) command: `set /SYS/MB/P` x`/MR` y`/ clear_fault_action=true` Where `P` x`/MR` y identifies the riser the fault was reported against. If the fault recurs, contact your Oracle service representative.

Previous
Next