Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 2.4 Positioning the Server for Maintenance

To remove and replace components in the Sun Fire X4470 Server, you must extend the server to the maintenance position.

## Extend the Server to the Maintenance Position

1. Verify that no cables will be damaged or will interfere when the server is extended.

   Although the cable management arm (CMA) that is supplied with the server is hinged to accommodate extending the server, you should ensure that all cables and cords are capable of extending.

2. From the front of the server, release the two slide release latches (Slide Release Latch).

   Squeeze the green slide release latches to release the slide rails.

   Figure 2-2 Slide Release Latch

3. While squeezing the slide release latches, slowly pull the server forward until the slide rails latch.

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |