Go to main content
oracle home

# Sun Fire X4470 Server Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: September 2018

- Sun Fire X4470 Server Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Sun Fire X4470 Product Notes

- Server Security, Software Releases, and Critical Patch Updates

- IMPORTANT - Install Latest OS Updates, Patches, and Firmware

- Changes to TLSv1.1 Configuration Property as of ILOM 4.0.3.x
- Oracle ILOM File Transfer Using URI Fails if Target Password Contains Special Characters (25917655)
- Diagnosing SAS Data Path Failures on Servers Using MegaRAID Disk Controllers
- Deprecation Notice for Oracle ILOM IPMI 2.0 Management Service
- Resolving Warning Messages for Custom CA and Self-Signed SSL Certificates
- Oracle ILOM License Information
- Supported Operating Systems
- Supported Operating Systems
- Supported Operating Systems in Software Releases
- Available Preinstalled Operating Systems
- Oracle Unbreakable Enterprise Kernel for Linux
- Supported Firmware and Software
- Supported Firmware in Software Releases
- Firmware Updates
- Supported Software
- Downloading an OS or Software Applications
- Supported PCIe Cards
- Quantity and Slot Restrictions
- Minimum Firmware Revisions for PCIe Cards
- Sun Flash Accelerator F20 PCIe Card Requirements
- Card Placement and Cooling
- ESM Replacement Interval
- Internal Sun Storage 6Gb SAS PCIe RAID HBA Requirements
- Sun Storage 10GbE FCoE PCIe Low Profile Dual Port CNA and OS Support
- Oracle x86 Products Accessibility

- Hardware Accessibility
- Oracle ILOM Accessibility
- Oracle Hardware Management Pack Accessibility
- BIOS Accessibility
- Documentation Accessibility

- Known Open Issues
- Hardware Known Issues
- Firmware Known Issues
- BIOS Known Issues
- Oracle ILOM Known Issues
- Oracle Solaris Known Issues
- Oracle Linux, SUSE Linux Enterprise Server (SLES), Red Hat Enterprise Linux (RHEL), and Oracle VM Known Issues
- Windows Known Issues
- Documentation Known Issues
- Broken Links in Sun Server X4470 Documentation Library
- Getting Firmware and Software Updates

- Firmware and Software Updates
- Options for Accessing Firmware and Software Updates
- Software Releases
- Getting Updates From Oracle Hardware Installation Assistant or My Oracle Support
- Download Firmware and Software Updates From My Oracle Support
- Installing Updates Using Other Methods
- Oracle Support

Language:

### Internal Sun Storage 6Gb SAS PCIe RAID HBA Requirements

If you are using the internal Sun Storage 6Gb SAS PCIe RAID host bus adapter (HBA) (SGX-SAS6-R-INT-Z or SG-SAS6-R-INT-Z), your configuration must meet the following requirements for proper battery cooling:

- The HBA must be installed in PCIe slot 4. In slot 4, the battery on the HBA faces an area with greater airflow, which is required for proper battery cooling. Do not move the HBA to slot 2 to allow slot 3 to operate in x16 mode.

- With this HBA installed, the ambient temperature requirement for the server is as follows:

  - Operating temperature: 5 oC to 32 oC (41 oF to 89.6 oF)

    Note - In Software Releases prior to Software Release 1.2.1, when this HBA is installed in the server, the Enhanced PCIe Cooling Mode Policy must be enabled in Oracle ILOM. As of Software Release 1.2.1, this Oracle ILOM policy is no longer required.

Previous
Next