Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## A.3 Environmental Requirements

Environmental Requirements lists the environmental requirements for the server.

Table A-3 Environmental Requirements

Parameter | Value
--- | ---
Operating temperature (single, non-rack system) | 5o C to 35o C (41o F to 95o F)
Nonoperating temperature (single, non-rack system) | -40o C to 70o C (-40o F to 158o F)
Operating humidity (single, non-rack system) | 10% to 90% relative humidity, non-condensing
Nonoperating humidity (single, non-rack system) | Up to 93% relative humidity, non-condensing
Altitude (operating) (single, non-rack system) | Up to 3048 m, maximum ambient temperature is derated by 1 degree C per 300 m above 900 m
Altitude (nonoperating) (single, non-rack system) | Up to 12,000 m

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |