Go to main content
oracle home

# Sun Fire X4470 Server Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: September 2018

- Sun Fire X4470 Server Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Sun Fire X4470 Product Notes

- Server Security, Software Releases, and Critical Patch Updates

- IMPORTANT - Install Latest OS Updates, Patches, and Firmware

- Changes to TLSv1.1 Configuration Property as of ILOM 4.0.3.x
- Oracle ILOM File Transfer Using URI Fails if Target Password Contains Special Characters (25917655)
- Diagnosing SAS Data Path Failures on Servers Using MegaRAID Disk Controllers
- Deprecation Notice for Oracle ILOM IPMI 2.0 Management Service
- Resolving Warning Messages for Custom CA and Self-Signed SSL Certificates
- Oracle ILOM License Information
- Supported Operating Systems
- Supported Operating Systems
- Supported Operating Systems in Software Releases
- Available Preinstalled Operating Systems
- Oracle Unbreakable Enterprise Kernel for Linux
- Supported Firmware and Software
- Supported Firmware in Software Releases
- Firmware Updates
- Supported Software
- Downloading an OS or Software Applications
- Supported PCIe Cards
- Quantity and Slot Restrictions
- Minimum Firmware Revisions for PCIe Cards
- Sun Flash Accelerator F20 PCIe Card Requirements
- Card Placement and Cooling
- ESM Replacement Interval
- Internal Sun Storage 6Gb SAS PCIe RAID HBA Requirements
- Sun Storage 10GbE FCoE PCIe Low Profile Dual Port CNA and OS Support
- Oracle x86 Products Accessibility

- Hardware Accessibility
- Oracle ILOM Accessibility
- Oracle Hardware Management Pack Accessibility
- BIOS Accessibility
- Documentation Accessibility

- Known Open Issues
- Hardware Known Issues
- Firmware Known Issues
- BIOS Known Issues
- Oracle ILOM Known Issues
- Oracle Solaris Known Issues
- Oracle Linux, SUSE Linux Enterprise Server (SLES), Red Hat Enterprise Linux (RHEL), and Oracle VM Known Issues
- Windows Known Issues
- Documentation Known Issues
- Broken Links in Sun Server X4470 Documentation Library
- Getting Firmware and Software Updates

- Firmware and Software Updates
- Options for Accessing Firmware and Software Updates
- Software Releases
- Getting Updates From Oracle Hardware Installation Assistant or My Oracle Support
- Download Firmware and Software Updates From My Oracle Support
- Installing Updates Using Other Methods
- Oracle Support

Language:

### Quantity and Slot Restrictions

Figure 3, Table 3, PCIe Card Quantity and Slot Restrictions lists the quantity and slot restrictions for PCIe cards supported on the Sun Fire X4470 Server server. The Maximum Quantity Supported column indicates the number of cards tested and supported by Oracle.

Table 3 PCIe Card Quantity and Slot Restrictions
PCIe Card | Maximum Quantity Supported | Slot Restrictions
--- | --- | ---
Sun Flash Accelerator F20 PCIe Card TA-FAS-S3IE96GB-N XTA-FAS-S3IE96GB-N | 4 | Supported in slots 9, 4, 8, 7, or 6 only.
Sun Storage 10GbE FCoE PCIe Low Profile, Dual Port Twin-Ax Converged Network Adapter SG-PCIEFCOE2-Q-TA SG-XPCIEFCOE2-Q-TA | 4 | Supported in all slots except x4 electrical interface slots (slots 0 and 9).
Sun Storage 10GbE FCoE PCIe Low Profile, Dual Port SR Converged Network Adapter SG-PCIEFCOE2-Q-SR SG-XPCIEFCOE2-Q-SR | 4 | Supported in all slots except x4 electrical interface slots (slots 0 and 9).
Sun Storage 6Gb SAS PCIe RAID HBA, Internal SGX-SAS6-R-INT-Z SG-SAS6-R-INT-Z | 1 | Supported in slot 4 only. See Internal Sun Storage 6Gb SAS PCIe RAID HBA Requirements for more information.
Sun Storage 6Gb SAS PCIe HBA, Internal SGX-SAS6-INT-Z SG-SAS6-INT-Z | 1 | Supported in slot 2.
Sun Storage 6Gb SAS PCIe HBA, External SGX-SAS6-EXT-Z SG-SAS6-EXT-Z | 4 | Supported in all slots except x4 electrical interface slots (slots 0 and 9).
8Gb Single FC PCI-Express, QLogic SG-PCIE1FC-QF8-Z SG-XPCIE1FC-QF8-Z | 8 | Supported in all slots.
8Gb Dual FC PCI-Express, QLogic SG-PCIE2FC-QF8-Z SG-XPCIE2FC-QF8-Z | 8 | Supported in all slots.
8Gb Single FC PCI-Express, Emulex SG-PCIE1FC-EM8-Z SG-XPCIE1FC-EM8-Z | 8 | Supported in all slots.
8Gb Dual FC PCIE-Express, Emulex SG-PCIE2FC-EM8-Z SG-XPCIE2FC-EM8-Z | 8 | Supported in all slots.
Sun PCI-Express Quad Gigabit Ethernet UTP Low Profile Adapter 4446A-Z-N X4446A-Z-N | 8 | Supported in all slots.
Sun Dual 10GbE SFP+ PCIe 2.0 Low Profile Adapter 1109A-Z X1109A-Z | 6 (Software Release 1.2.1) 2 (Software Release 1.0 and 1.1) | Supported in all slots except x4 electrical interface slots (slots 0 and 9). Note – Six cards supported as of Software Release 1.2.1. Two cards supported as of Software Releases 1.0 and 1.1.
InfiniBand Quad Data Rate PCIe Adapter X4242A | 4 | Supported in all slots except x4 electrical interface slots (slots 0 and 9).
InfiniBand Quad Data Rate PCIe Host Channel Adapter 4237A-N X4237A-N | 4 (Software Release 1.3) 2 (Software Release 1.0 and 1.1) | Supported in all slots except x4 electrical interface slots (slots 0 and 9). Note – Four cards supported as of Software Release 1.3. Two cards supported as of Software Releases 1.0 and 1.1.

Previous
Next