Go to main content
oracle home

# Sun Fire X4470 Server Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: September 2018

- Sun Fire X4470 Server Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Sun Fire X4470 Product Notes

- Server Security, Software Releases, and Critical Patch Updates

- IMPORTANT - Install Latest OS Updates, Patches, and Firmware

- Changes to TLSv1.1 Configuration Property as of ILOM 4.0.3.x
- Oracle ILOM File Transfer Using URI Fails if Target Password Contains Special Characters (25917655)
- Diagnosing SAS Data Path Failures on Servers Using MegaRAID Disk Controllers
- Deprecation Notice for Oracle ILOM IPMI 2.0 Management Service
- Resolving Warning Messages for Custom CA and Self-Signed SSL Certificates
- Oracle ILOM License Information
- Supported Operating Systems
- Supported Operating Systems
- Supported Operating Systems in Software Releases
- Available Preinstalled Operating Systems
- Oracle Unbreakable Enterprise Kernel for Linux
- Supported Firmware and Software
- Supported Firmware in Software Releases
- Firmware Updates
- Supported Software
- Downloading an OS or Software Applications
- Supported PCIe Cards
- Quantity and Slot Restrictions
- Minimum Firmware Revisions for PCIe Cards
- Sun Flash Accelerator F20 PCIe Card Requirements
- Card Placement and Cooling
- ESM Replacement Interval
- Internal Sun Storage 6Gb SAS PCIe RAID HBA Requirements
- Sun Storage 10GbE FCoE PCIe Low Profile Dual Port CNA and OS Support
- Oracle x86 Products Accessibility

- Hardware Accessibility
- Oracle ILOM Accessibility
- Oracle Hardware Management Pack Accessibility
- BIOS Accessibility
- Documentation Accessibility

- Known Open Issues
- Hardware Known Issues
- Firmware Known Issues
- BIOS Known Issues
- Oracle ILOM Known Issues
- Oracle Solaris Known Issues
- Oracle Linux, SUSE Linux Enterprise Server (SLES), Red Hat Enterprise Linux (RHEL), and Oracle VM Known Issues
- Windows Known Issues
- Documentation Known Issues
- Broken Links in Sun Server X4470 Documentation Library
- Getting Firmware and Software Updates

- Firmware and Software Updates
- Options for Accessing Firmware and Software Updates
- Software Releases
- Getting Updates From Oracle Hardware Installation Assistant or My Oracle Support
- Download Firmware and Software Updates From My Oracle Support
- Installing Updates Using Other Methods
- Oracle Support

Language:

### Card Placement and Cooling

If you are using the Sun Flash Accelerator F20 PCIe card, your configuration must meet the following requirements for proper installation and cooling:

- Do not connect devices to the internal SAS/SATA ports of the Sun Flash Accelerator F20 PCIe card. The Sun Fire X4470 does not support using this card as an internal host bus adapter (HBA).

- The HBA can be installed only in PCIe slots 9, 4, 8, 7, or 6, in that order of preference (slot 9 is the preferred slot to use for this HBA and slot 6 is acceptable but is the least desirable slot to use).

  Note - If you are using a Sun Storage 6Gb SAS PCIe RAID HBA, that HBA must be installed in slot 4; therefore, slot 4 will not be available for the Sun Flash Accelerator F20 PCIe card.

- If you are using the Sun Flash Accelerator F20 PCIe card, you must use the Oracle Integrated Lights Out Manager (ILOM) available with Software Release 1.2.1 or later.

- With this HBA installed only in slots 9 and/or 4, the ambient temperature requirement for the server remains as follows:

  - Operating temperature: 5 oC to 35 oC (41 oF to 95 oF)

  - Nonoperating temperature: -40 oC to 70 oC (-40 oF to 158 oF)

- With this HBA installed in slot 8, slot 7, or slot 6, the ambient temperature requirement for the server is modified to the following:

  - Operating temperature: 5 oC to 32 oC (41 oF to 89.6 oF)

Previous
Next