Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 1.3 Server Back Panel Features

Server Back Panel Features shows the Sun Fire X4470 Server back panel and describes its components.

Figure 1-6 Server Back Panel Features

Figure Legend

1 Power supply unit 0 status indicator LEDs: Service action required: amber DC OK: green AC OK: green or amber

2 Power supply unit 0 AC inlet

3 Power supply unit 1 status indicator LEDs: Service action required: amber DC OK: green AC OK: green or amber

4 Power supply unit 1 AC inlet

5 system status LEDs, location ofcluster card slot, location ofSystem status LEDs: Power/OK: green Service action required: amber Locate: white

6 PCIe card slots 0–4

7 Cluster card slot

8 network management ports, location ofNetwork (NET) 10/100/1000 ports: NET0–NET3

9 USB connectorlocation ofUSB 2.0 connectors (2)

10 PCIe card slots 5–9

11 Service processor (SP) network management (NET MGT) port

12 serial connection, location ofSerial management (SER MGT)/RJ-45 serial port

13 video connectorlocation ofDB-15 video connector

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |