Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 4.3 Servicing the DVD Drive and DVD Driver Filler Panel (CRU)

Use the following procedures to remove and replace the DVD drive and DVD drive filler panel.

## Remove the DVD Drive or DVD Drive Filler Panel

Refer to Removing the DVD Drive or Filler Panel when completing the following procedure.

1. Prepare for servicing:
   1. Attach an antistatic wrist strap.

      See 2.3 Performing Electrostatic Discharge and Static Prevention Measures.

   2. Remove any media from the drive.
   3. Power off the server.

      See 2.6 Powering Off the Server.

2. Push down on the latch on the top left corner of the DVD drive or filler panel.
3. Slide the DVD drive or filler panel out of the server.

   | Caution - Whenever you remove the DVD drive or filler panel, you should replace it with another DVD drive or a filler panel; otherwise the server might overheat due to improper airflow.

   Figure 4-11 Removing the DVD Drive or Filler Panel

## Install the DVD Drive or DVD Drive Filler Panel

Refer to Installing the DVD Drive or Filler Panel when completing the following procedure.

1. Unpack the DVD drive or filler panel.

   If it is a DVD drive, place it on an antistatic mat.

2. Slide the DVD drive or filler panel into the front of the chassis until it seats.

   Figure 4-12 Installing the DVD Drive or Filler Panel

3. Return the server to operation:
   1. Return the server to the normal rack position.

      See 6.2 Returning the Server to the Normal Rack Position.

   2. Power on the server.

      See 6.3 Powering On the Server.

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |