Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 1.1 System Overview

Oracle’s Sun Fire X4470 Server is a 3 rack unit (RU) rackmount server that uses the Intel Xeon 7500 platform. This section describes the major features, components, and capabilities of the server.

### 1.1.1 Intel Xeon 7500 Platform

The Intel Xeon 7500 platform is based on the Intel Xeon Processor 7500 Series and uses the Intel 7500 Chipset I/O hub (IOH) as its primary chipset. The platform uses the Intel QuickPath Interface (QPI), a high-speed, differentially signaled, point-to-point interface that forms a communication fabric among the CPUs and IOHs in the system.

The Sun Fire X4470 Server uses two Intel 7500 Chipset I/O hubs, each connected to two of the four CPUs. One of these I/O hubs is designated the legacy I/O hub and has a connection to the Intel I/O Controller Hub 10 (ICH10) southbridge component.

### 1.1.2 Block Diagrams

Four CPU Block Diagram shows a block diagram for a Sun Fire X4470 Server with four CPUs.

Two CPU Block Diagram shows a block diagram for a Sun Fire X4470 Server with two CPUs.

Note - In the diagrams, the PCIe SAS/RAID Controller is shown as installed in Slot 2. If a particular SAS/RAID Controller has specific cooling requirements, it might have to be installed in Slot 4. For information about cooling requirements, refer to the Sun Fire X4470 Server Product Notes (820-0704).

Figure 1-1 Four CPU Block Diagram

Figure 1-2 Two CPU Block Diagram

### 1.1.3 CPUs

The Sun Fire X4470 Server supports two or four CPUs, as shown in Four CPU Block Diagram and Two CPU Block Diagram. The two-CPU configuration must have CPUs (with heatsinks) in sockets 0 and 2 and heatsink filler panels installed in sockets 1 and 3.

In a two-CPU configuration, all three QPI interconnects and both CPUs must be operational. The four-CPU configuration offers a greater level of resiliency with redundant QPI interconnects that allow working CPUs to route around a disabled CPU as the system starts.

Features of each Intel Xeon Processor 7500 Series include:

- Up to eight cores with Hyper-Threading (two threads/core)

- Up to 24MB shared last level cache

- 45nm process technology

- Two integrated memory controllers with four Intel Scalable Memory Interconnects (SMI channels)

  - Supports speeds of DDR3-800, 978 and 1067 MT/s via an Intel 7500 Scalable Memory Buffer

- Four full-width, bidirectional Intel QuickPath interconnects (QPI links)

  - 4.8, 5.86, or 6.4 GT/s (9.6 to 12.8 GB/s per direction)

  - Automatic self-healing by degrading to half-width or quarter-width link operation

- CPU Thermal Design Power (TDP) of 130W, 105W, or 95W

### 1.1.4 Memory

Each CPU in the Sun Fire X4470 Server has four SMI channels leading to Intel 7500 Scalable Memory Buffers (located on two memory risers). Each memory buffer has an SMI link to the CPU and two DDR3 interfaces. Each SMI interface can operate at speeds of 4.8, 5.86, and 6.4 GT/s, which correspond to DDR3 operation at 978 or 1067 MT/s. From the CPU to the Intel 7500 Scalable Memory Buffer, the SMI interface supports 11 lanes (9 data + 1 CRC + 1 spare). From the Intel 7500 Scalable Memory Buffer to the CPU, the SMI interface supports 14 lanes (12 data + 1 CRC + 1 spare). The CPU retries memory transactions that incur a CRC error. For persistent errors, the SMI link has spare lanes for automatic self-healing.

The system supports a maximum of eight memory risers (4 CPU configuration) or four memory risers (2 CPU configuration). Each riser houses 8 DIMM slots for the four DDR3 channels. The system can operate with 0, 2, 4, 6 or 8 DIMMs on a given riser. For maximum performance, install at least two ranks of DIMMs on every available DDR3 channel (for example, 4 DIMMs per riser with two risers per CPU).Each of two memory controllers in a CPU operates its two SMI channels as a lock-step pair. The memory controller treats each pair of DDR3 channels behind the two memory buffers as a 144-bit-wide DRAM interface. As a result, the DIMMs must be installed in pairs, with identical DIMMs in each pair.

The DDR3 interfaces include the following features:

- Accommodates x4 and x8 Single-Rank, Dual-Rank, Quad-Rank RDIMMs (Single-Rank and Quad-Rank DIMMs are not currently offered with the server.)

- Supports up to 2 RDIMMs per DDR3 channel (8 DIMM slots per memory riser)

- DDR3 speeds: 978 or 1067 MT/s (dictated by SMI speeds of CPUs)

- DRAM Technology: 1 or 2 GB die, 1.5-volt operation

- DIMM Capacity: 2, 4, 8, 16 GB (16 GB with QR DIMMs only)

  - Currently supported DIMMs are dual-rank in 2-, 4-, and 8-GB sizes

For more information about CPUs, memory risers, and memory layout, including guidelines for populating memory risers and DIMMs, see 4.1 Servicing Memory Risers and DIMMs (CRU).

Memory Architecture shows the architecture of the server memory.

Figure 1-3 Memory Architecture

### 1.1.5 Cooling

The Sun Fire X4470 Server is cooled from front to back. Cooling occurs in two areas of the chassis, separated by a plastic dividing wall. In the power supply cooling zone, fans at the back of the power supplies cool the drive bays as well as the power supplies, by drawing air into the depressurized zone at the right of the chassis. In the main cooling zones, six 92-mm high-performance fans, arranged in two rows for redundancy, cool the motherboard, memory risers, and I/O cards. The motherboard is divided into three zones and each pair of fans is separately regulated to cool that zone. Since the main cooling zones are pressurized, it is important to maintain the seal of the dividing wall so that the power supply units can draw air through the drive bay.

The unrestricted airflow over the motherboard minimizes system noise. Dividing the cooling into zones allows for greater use of system resources, since each zone can operate independently at its highest efficiency.

Server Cooling Zones shows the cooling zones.

Figure 1-4 Server Cooling Zones

Figure Legend

1 Power supply cooling zone

2 Chassis cooling zone 2

3 Chassis cooling zone 1

4 Chassis cooling zone 0

### 1.1.6 Input/Output (I/O)

For internal storage, the server chassis provides:

- Six 2.5-inch drive bays, accessible through the front panel. The supported drive interfaces for each bay depend on the HBA chosen.

- An optional slot-loading DVD+/-RW drive on front of the server, below the drive bays. This SATA DVD connects to a USB-SATA bridge, so that is appears to the system software as a USB storage device.

- One internal high-speed USB port on the motherboard. This port can hold a USB flash device for system booting.

In addition, the service processor can present virtual USB storage devices to the system.The ICH10 southbridge on the motherboard provides six built-in SATA2 (3-Gbit/s) ports, accessible through two SAS4I connectors (Port 0-3 and Port 4-5). When configured with any 2.5-inch SAS drives, the system must be equipped with one PCI Express (PCIe) Gen-2 internal HBA card to support the front 2.5-inch drive bays.Each offered PCIe Gen-2 HBA has 8 SAS2/SATA2 internal ports accessible through two SAS4I connectors (Port 0-3 and Port 4-7). Since the drive cage has only six bays, Port 6-7 of an internal HBA are not used in this system.

With an internal SAS-2 HBA card installed in a PCIe slot, the six bays can handle any combination of supported SAS and SATA hard disk drives (HDDs) and solid-state drives (SSDs). If the disk backplane is connected to the built-in ICH10 SATA-2 controller rather than an HBA card, only SATA storage devices will operate. (When a RAID volume is configured on the HBA card, the drive bays for the RAID members must hold the same type of storage device.)

### 1.1.7 Summary of Supported Components and Capabilities

The following table summarizes the components and capabilities of the Sun Fire X4470 Server.

Table 1-1 Sun Fire X4470 Server Components and Capabilities

Component | X4470 Server
--- | ---
CPU | Supported configurations: Two processors installed in socket 0 and socket 2 Four processors installed in sockets 0 through 3 For the latest information on CPU specifications, go to http://www.oracle.com/technetwork/server-storage/sun-x86/overview/index.html and navigate to the applicable web site.
Memory | Up to eight memory riser modules are supported (two risers per CPU) in the server chassis. Each riser module supports eight RDIMMs, allowing up to sixteen RDIMMs per processor. A 2-socket system using four riser modules populated with 8-GB RDIMMs supports a maximum of 256 GB of system memory. A 4‐socket system using eight riser modules populated with 8-GB RDIMMs supports a maximum of 512 GB of system memory.
Storage devices | For internal storage, the server chassis provides: Six 2.5-inch drive bays, accessible through the front panel. The supported drive interfaces for each bay depend on the HBA chosen. An optional slot-loading DVD+/-RW drive on front of the server, below the drive bays. This SATA DVD connects to a USB-SATA bridge, so that is appears to the system software as a USB storage device. One internal high-speed USB port on the motherboard. This port can hold a USB flash device for system booting.
USB 2.0 ports | Two front, two rear, and one internal
VGA ports | One front and one rear high-density DB-15 video ports. Note - The rear VGA port supports VESA Device Data Channel for monitor identification.
PCI Express 2.0 I/O slots | Ten PCI Express 2.0 slots that accommodate low-profile PCIe cards. All slots support x8 PCIe connectors. Two slots are also capable of supporting x16 PCIe connectors. Slots 0 and 9: x4 electrical interface Slots 1, 2, 4, 6, 7, and 8: x8 electrical interface Slots 3 and 5: x8 or x16 electrical interface (x16 connector) Note - PCI Express slots 3 and 5 will operate as x16 interfaces only when an x16 capable card is installed and the adjacent slot (4 or 6) is unpopulated.
Cluster card slot | One specialized slot dedicated for use in storage appliances. The Sun Fire X4470 Server does not support populating this slot with standard PCIe cards.
PCI Express I/O cards | For a list of I/O cards that are customer-orderable options, go to http://www.oracle.com/technetwork/server-storage/sun-x86/overview/index.html and navigate to the applicable web site.
Ethernet ports | Four 10/100/1000 RJ-45 GbE ports on rear panel Each Network Interface Controller (NIC) supports Intel QuickData Technology, Intel I/OAT, VMDq, PCI-SIG SR-IOV, IPSec offload, and LinkSec.
Service processor | Integrated Baseboard Management Controller (BMC), which supports the industry-standard IPMI feature set. Supports remote KVM, DVD and floppy over IP (optional license required). Includes serial port. Supports Ethernet access to SP through a dedicated 10/100BaseT management port and optionally through one of the host GbE ports (sideband management).
Power supplies | Two hot-swappable power supplies, each with 2000 Watts capacity (from 200 Volts to 240 Volts), auto-ranging, light load efficiency mode and redundant over-subscription.
Cooling fans | Six hot-swappable, redundant fans at chassis front (top-loading); redundant fans at each power supply.
Management software | Oracle Integrated Lights Out Manager (ILOM)

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |