Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## C.3 Gigabit-Ethernet Connectors

Four RJ-45 Gigabit-Ethernet connectors (NET0, NET1, NET2, NET3) can be accessed from the back panel. The Ethernet interfaces operate at 10 Mbit/sec, 100 Mbit/sec, and 1000 Mbit/sec.

Figure C-3 Gigabit Ethernet Connector

Figure Legend

1 Transmit/Receive Data 0 +

2 Transmit/Receive Data 0 –

3 Transmit/Receive Data 1 +

4 Transmit/Receive Data 2 +

5 Transmit/Receive Data 2 –

6 Transmit/Receive Data 1 –

7 Transmit/Receive Data 3 +

8 Transmit/Receive Data 3 –

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |