Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 6.2 Returning the Server to the Normal Rack Position

If you extended the server to the maintenance position, use the following procedure to return the server to the normal rack position.

## Return the Server to the Normal Rack Position

Refer to Inserting Server Back Into Rack when completing the following procedure.

1. Release the slide rails from the fully extended position by pushing the release tabs on the side of each rail.

   Figure 6-2 Inserting Server Back Into Rack

2. While pushing on the release tabs, slowly push the server into the rack.

   Ensure that the cables do not get in the way.

3. Reconnect the cables to the back of the server.

   If the cable management arm (CMA) is in the way, disconnect the left CMA release and swing the CMA open.

4. Reconnect the CMA.

   Swing the CMA closed and latch it to the left rack rail.

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |