Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 6.1 Replacing the Server Top Cover

When you have completed a service procedure, replace the server top cover, using the following procedure.

## Replace the Server Top Cover

Refer to Installing the Top Cover when completing the following procedure.

1. Place the top cover on the chassis.

   Set the cover down so that it is slightly forward of the rear of the server by about 1 inch (25.4 mm).

2. Slide the top cover toward the rear of the chassis until the rear cover lip engages with the rear of the chassis.
3. To close the top cover, press down on the cover with both hands until both latches engage.

   Figure 6-1 Installing the Top Cover

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |