Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## A.2 Electrical Specifications

Electrical Specifications lists the electrical specifications for the server.

Table A-2 Electrical Specifications

Parameter | Value
--- | ---
Input:
Nominal frequencies | 50/60 Hz
AC operating voltage range | 100-127 VAC for 2 CPUs 200-240 VAC for 2 or 4 CPUs
Maximum current AC RMS | 12A @ 100 VAC / 12A @ 200 VAC
Power dissipation:
Max power consumption | 1800 W
Max heat output | 6143 BTU/hr
Volt-Ampere rating | 1837 VA @ 240 VAC, 0.98 P.F.

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |