Index

### A

AMC

devices, 1

installing, 1

AMC I/O, 1

`auto-boot` (OpenBoot configuration variable), 1

automatic system recovery (ASR)

disabling, 1

enabling, 1

### B

barcode labels, locating, 1

board layout, 1

### C

cabling, 1

collecting network information, 1

compliance

NEBS, 1

PICMG specifications, 1

components, 1

configurations

I/O configurations, 1

### D

descriptions<endrange>, 1

descriptions<startrange>, 1

device

information, retrieving, 1

device paths, hardware, 1

diagnostics

POST, 1

SunVTS software, 1

DIMM memory module

described, 1

installing, 1

removing, 1

requirements, 1

### E

electric shock caution, 1

error handling, summary, 1

Ethernet

RJ-45, 1

### F

features, 1

CPU, 1

hot-swap, 1

memory, 1

power requirements, 1

Flash update, 1

form factor, 1

front panel, 1, 2

connections, 1

frutree

entries and properties, 1

hierarchy, 1

fuses, 1

### G

graceful system halt, 1

### H

halt, gracefully, advantages of, 1

hardware, 1, 2

hardware architecture, 1

hardware device paths, 1

hardware installation, 1 - 2

AMC device, 1

collecting network information, 1

DIMM modules, 1

preparation, 1

summary, 1

tools needed, 1

hot-swap

information, 1

LED indicator, 1

support, 1

### I

I/O connections

front panel, 1

IDE bus, 1

`init` (Solaris command), 1

installation

AMC device, 1

DIMM modules, 1

overall procedure, 1

preparation, 1

tools needed, 1

installing

rear transition modules, 1

integrated drive electronics (IDE)

Intelligent Platform Management controller (IPMC), 1

Internet Assigned Numbers Authority (IANA), 1

IPMC (Intelligent Platform Management controller), 1

IPMI system management, 1

### L

LED

hot-swap, 1

LEDs

Active, 1

Fault, 1

front panel, 1

hot swap, 1

### M

MAC address, 1

label, 1

manual system reset, 1

memory, 1

DIMM

module, 1

message

POST, error, 1, 2

### N

netfunction (NetFn), 1

### O

`ok` prompt

ways to access, 1

OpenBoot commands

`probe-ide`, 1

`show-devs`, 1

OpenBoot configuration variables

`auto-boot`, 1

### P

part number, locating, 1

PICL, 1

pinouts

serial port, 1

platform information and control library (PICL), 1

POST

error messages, 1, 2

See also POSTpower-on self-test (POST), 4-2

power

requirements, 1

power module, 1

power-on self-test (POST)

See POST

power-on sequence, 1

preparation

installation, 1

`probe-ide` command (OpenBoot), 1

PROM contents, 1

### R

rear transition module, features, 1

removing DDR-2 DIMM module, 1

requirements

hardware, 1

safety, 1

software, 1, 2

reset

manual system, 1

scenarios, 1

RJ-45 Ethernet, 1

RTM (rear transition module), 1

### S

serial

number, locating, 1

port, 1

`show-devs` command, OpenBoot, 1

`shutdown` (Solaris command), 1

software

hot-swap

information, 1

PICL, 1

requirements, 1

Solaris commands

`init`, 1

`shutdown`, 1

Sun OEM IPMI commands, 1

`Get RTM Status`, 1

`Get Version`, 1

Sun Services, 1

SunVTS software, 1

support, contacting, 1

system reset scenarios, 1

### T

TOD clock

battery, 1, 2

battery holder, 1

tools needed, 1

### W

warranty, 1

watch-net, 1

Copyright © 2009 Sun Microsystems, Inc. All rights reserved.