C H A P T E R 2

Overview

This chapter introduces the key features of the AMC. This chapter includes a product definition, a list of product features, and functional block diagrams with brief descriptions. This chapter can be used to compare the features of the AMC against the needs of a specific application.

This chapter contains the following topics:

- Section 2.1, Features

- Section 2.2, Key Components

- Section 2.3, Faceplate and LEDs

- Section 2.4, Functional Diagram

- Section 2.5, Technical Support and Warranty

- Section 2.6, Part Number, Serial Number, and Revision Number Identification

- Section 2.7, Disposal

##

2.1 Features

Part of Sun’s ATCA platform, the Sun Netra CP3000 AMC.1-HDD SAS disk complies with PICMG 3.0 AdvancedTCA Specification R2.0 ECN002 and the following specifications:

- PICMG AMC.0 Rev. 2.0

- AMC.1 Revision 1, PCI Express option

- AMC.3 Revision 1, storage signaling option

The AMC.1-HDD SAS disk is an Advanced Mezzanine Card (AMC) that integrates both an SAS hard drive disk and a x4 PCIe SAS controller. Occupying only one AMC site, the highly integrated combination provides embedded systems designers the ability to add an Enterprise SAS Hard Disk Drive (HDD) to a system that does not have native SAS connectivity. The AMC.1-HDD SAS disk is offered as a single-width AMC, with options for mid- or full-height panels. The hard drive is Form-Factor 2.5” to provide the greatest spindle density for ATCA applications.

The AMC.1-HDD SAS disk plugs into ATCA carrier blades that support a combination of AMC.1 (PCI Express) and AMC.3 (SAS) storage signaling.

The AMC.1-HDD SAS disk includes a modular management controller (MMC).

This AMC is designed for use in a wide variety of next-generation and wireless-networking equipment. Designed for high performance and reliability, the AMC.1-HDD SAS disk is ideal for telecommunications equipment manufacturers (TEMs) and OEMs. TEMs can add SAS connectivity to networking equipment that uses the ATCA platform specification. OEMs can design to the MicroTCA specification for high-performance embedded systems.

The following briefly outlines the features of the AMC.1-HDD SAS disk:

- Advanced Mezzanine Card (single-width, mid- or full-height); PICMG AMC.0 compliant

- Hot-swappable

- PCI Express interface (auto configure x1 or x4 lanes at 2.5 Gigabits per second

- One Integrated 2.5” SAS hard drive (primary port)

- Additional disk via AMC.3 storage signaling (drives adjacent site AMC port 2)

- Additional disk via AMC.3 storage signaling (drives adjacent site AMC port 3)

- All SAS links at 3 Gigabits per second maximum

- Support for SSP, STP, and SMP, as defined in the Serial Attached SCSI (SAS) Specification, version 1.0

- Drive over-current protection

- Support for SATA, as defined in the Serial ATA Specification, version 1.0a.

##

2.2 Key Components

The following figure and sections describe key components of the Sun Netra CP3000 AMC.1-HDD SAS disk.

FIGURE 2-1 Top-Level AMC Layout

### 2.2.1 Hard Drive Disk

The Sun Netra CP3000 AMC.1-HDD SAS disk provides a single SAS hard drive, with various capacity options available. When you order the product, choose the part number corresponding to the capacity (in gigabytes) that you want.

### 2.2.2 Power Regulator

The power regulator is the part of the module that generates the required power from the payload power (+12V) that is delivered to the module through the AMC connector. This power is current-limited by the onboard regulator.

### 2.2.3 SAS Controller

The AMC.1-HDD SAS disk incorporates a PCIe-to-SAS host controller manufactured by LSI Corporation, device model LSI-SAS1064E. The controller provides host access to SAS and SATA disks. The controller features four lanes of PCI Express (2.5 gigabits per second each), and four lanes of SAS (3.0 gigabits per second each).

The SAS firmware for the LSI SAS supports the following:

- 3 gigabits per second SAS and SATA transfers

- Device discovery

- Both 3.0 gigabit and 1.5 gigabit SATA devices

- x1 or x4 PCI Express bus

- Mixed SAS and SATA disk operation

- SATA tape drive

- SAS expander compatibility

### 2.2.4 Flash

A flash device is preloaded with firmware that manages the protocols necessary to communicate with SAS and SATA target devices. The flash device contains BIOS and F-code to support boot from disk operations.

### 2.2.5 Module Management Controller (MMC)

The IPMI subsystem provides management control for the board, based on an Atmel microcontroller. The MMC is the first system component to be brought up and must negotiate with the carrier board over IPMI before the card payload is enabled.

The MMC monitors board voltages and temperature, controls the hot-swap and failures status LEDs, controls e-Keying, and stores FRU information. For more information about the MMC and management functions, see Chapter 3.

The MMC provides an Intelligent Platform Management Interface (IPMI) that communicates with AdvancedTCA shelf managers. This MMC controls and monitors the following:

- Hot-swap communication with the shelf manager

- Inlet air temperature

- Voltage monitoring

- e-Keying as described in the AMC.0 specification

- FRU information

- LED indicators for hot-swap and OOS (out of service)

### 2.2.6 Port Connectors

The AMC includes connectors to communicate with the host board and take its interfaces outside the ATCA chassis. Refer to Appendix A for complete connector descriptions and pin-outs.

### 2.2.7 LEDs

The AMC.1-HDD SAS disk has three LEDs. See the next section for a detailed description of the LEDs.

##

2.3 Faceplate and LEDs

The faceplate of the AMC.1-HDD SAS disk has three LED indicators, which are described in the table following the faceplate illustration.

Note - The AMC is available in different capacities (in gigabytes). The illustration shows a generic faceplate. For your product’s faceplate, the xxx denotes the capacity.

FIGURE 2-2 Faceplate

Figure Legend

| Indicator | Color | State | Description and Function
1 | OOS | Red | On | Out of Service: fault set by shelf manager, or 12V payload power not detected.
|  |  | Off | No module fault. 12V payload power is being supplied to board.
2 | OK | Green | On | Module in service. 12V payload power is being supplied to board.
|  |  | Off | 12V payload power is not detected.
3 | Hot Swap | Blue | On | Management power available to the module; AMC can be safely extracted.
|  |  | Off | The module is operational and is unsafe for extraction.
|  |  | Long blink | Delay before module is activated.
|  |  | Short blink | Delay before module is deactivated.

##

2.4 Functional Diagram

FIGURE 2-3 AMC SAS-HDD Functional Block Diagram

##

2.5 Technical Support and Warranty

If you have any technical questions or support issues that are not addressed in the Sun Netra CP3000 Advanced Mezzanine Card PCIe Hard Drive and SAS Controller documentation set or on the web site, contact your local Sun Services representative. This hardware carries a one-year return-to-depot warranty.

For customers in the US or Canada, call 1-800-USA-4SUN (1-800-872-4786).

For customers in the rest of the world, find the World Wide Solution Center nearest you by visiting our web site:

`http://www.sun.com/service/contacting/solution.html`

When you call Sun Services, indicate if the Sun Netra CP3000 AMC.1-HDD SAS disk was purchased separately and is not associated with a system. Have the proper AMC identification information ready. Be prepared to give the representative the AMC part number, serial number, and date code (FIGURE 2-4).

##

2.6 Part Number, Serial Number, and Revision Number Identification

The Sun Netra CP3000 AMC.1-HDD SAS disk part number, serial number, and revision can be found on labels located on the card (FIGURE 2-4). The Sun barcode labels provide the following information:

- `SunSN` - Sun serial number (for example, 1005LCB-0626WM001M)

- `SunPN` - Sun part number and dash number (for example, 501-7658-01), -01 is the dash number

- `Rev` - Revision number of the part (for example, Rev 06)

The Media Access Control (MAC) address label contains the MAC address for the blade server in printed and barcode form.

FIGURE 2-4 Sun Netra CP3000 AMC.1-HDD SAS disk Barcode Labeling

Figure Legend
1 | Final Assembly Number: Assembly process label, where xxx denotes disk drive capacity Rzz = Assembly Revision (Refer to Bill Of Material) where zz is a numeric revision
2 | Sub-Assembly Number: P/N = sub assembly Part Number 600-05101x
3 | Serial Number: S/N Format:AAA = Assembly Number (051) L =Location of manufacturer (S) Y = Calendar year of manufacturer (2008 = 8) MM = Calendar month of manufacturer (March = 03) SSSS = Sequence number (reset each month) (1234)
4 | Sun Product Label: SUN S/N Format Sun Part Number
5 | SAS WWN = SAS World Wide Name
6 | Safety label

##

2.7 Disposal

The AMC might contain materials that require regulation upon disposal. Please dispose of this product in accordance with local rules and regulations. For disposal or recycling information, please contact your local authorities or the Electronic Industries Alliance at `http://www.eiae.org/`.

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.