A P P E N D I X C

Agency Certifications

This appendix lists standards agencies and the certifications related to the Sun Netra CP3000 AMC.1-HDD SAS disk.

This product was tested in an EMC-compliant chassis and meets the requirements for EN55022 Class A equipment. Compliance was achieved under the following conditions:

- Conductive chassis rails connected to earth ground, providing the path for connecting shields to earth ground

- Front panel screws properly tightened

For minimum RF emissions, it is essential that these conditions be implemented. Failure to do so could compromise the EMC compliance of the equipment containing the module.

This appendix contains the following topics:

- Section C.1, CE Certification

- Section C.2, NEBS/ETSI

- Section C.3, Safety

- Section C.4, Emissions Test Regulations

- Section C.5, Regulatory Information

##

C.1 CE Certification

The Sun Netra CP3000 AMC.1-HDD SAS disk meets the intent of Directive 89/336/EEC for Electromagnetic Compatibility [EN55024:1998, EN55022:2006] and Low-Voltage Directive 73/23/EEC for Product Safety [EN60950-1:2001]. A certificate of incorporation is available upon request. The final system configuration must be reconsidered as a whole per these directives.

##

C.2 NEBS/ETSI

The Sun Netra CP3000 AMC.1-HDD SAS disk has been designed to meet or exceed:

- Telcordia specification SR-3580 Issue 3, June 2007

- Telcordia GR-63, Issue 3, March 2006, Network Equipment-Building System (NEBS) Requirements--Physical Protection

- Telcordia GR-1089, Issue 4, June 2006, Electromagnetic Compatibility And Electrical Safety Generic Criteria For Network Telecommunication Equipment

- ETSI EN 300 019-2-1 V2.1.2 (2000-09), -2-2 V2.1.1 (1999-09), -2-3 V2.2.2 (2003-04), Environmental conditions and environmental tests for telecommunication equipment; Part 2

- ETSI EN 300 119-5, V1.2.2 (2004-12), Part 4: Engineering requirements for subracks in miscellaneous racks and cabinets

- ETSI EN 300 132-2, September 1996, Equipment Engineering Power Supply Interface At The Input To Telecommunications Equipment; Part 2: Operated by direct current (DC

- ETSI EN 300 753, October 1997, Acoustic Noise Emitted By Telecommunications Equipment

Certification is dependent on your configuration.

##

C.3 Safety

- UL/cUL 60950--1 Safety for Information Technology Equipment (UL File #E138926)

- EN/IEC 60950-1:2001, 1ST ED CB/CCA -scheme, Safety for Information Technology Equipment (TUV CB certificate and report)

The following group and/or national deviations were considered:

- CENELEC Common Modifications, Annex ZA

- AU (Australia and New Zealand)

- CH (Switzerland)

- DE (Germany)

- DK (Denmark)

- ES (Spain)

- FI (Finland)

- GB (United Kingdom)

- IE (Ireland)

- KR (Korea)

- NO (Norway)

- SE (Sweden)

- China (deviations to IEC 60950 3rd Ed. considered):

- Telcordia GR-63-CORE Network Equipment-Building System (NEBS) Requirements Issue 3 Mar 2006--Physical Protection (Designed to meet section 4)

- Telcordia GR-1089-CORE Safety for Network Telecommunication Equipment Issue 4 Jun 2006 (meets Section 7)

##

C.4 Emissions Test Regulations

- FCC Part 15, Subpart B Class A Commercial Equipment

- Industry Canada ICES-003:2004 Class A Commercial Equipment

- CISPR 22/EN 55022:2006 Class A Radiated, Power line Conducted

- VCCI, Japanese V-3/2007.04 Class A

- Telcordia GR-1089-CORE EMC For Network Telecommunication Equipment Issue 4 Jun 2006 (Designed to meet Sections 2 and 3)

### C.4.1 EN 55022 Emissions

- Telcordia GR-1089-CORE EMC For Network Telecommunication Equipment Issue 4 Jun 2006 (designed to meet 3.2)

- EN55022:2005 Limits and Methods of Measurement of Radio Interference +A1:2000+A2:2003 Characteristics of Information Technology Equipment

- IEC CISPR22:2006 Limits and Methods of Measurement of Radio Interference Characteristics of Information Technology Equipment

- AS/NZS CISPR 22:2006 Limits and Methods of Measurement of Radio Disturbance Characteristics of Information Technology Equipment

### C.4.2 EN 55024 Immunity

- Telcordia GR-1089-CORE EMC For Network Telecommunication Equipment Issue 4 Jun 2006 (Sections 2.1 (ESD), designed to meet 2.2 (EFT), 3.3)

- EN 55024:1998 Information Technology Equipment - Immunity +A1:2001+A2:2003 characteristics limits and methods of measurements

- IEC 61000-4-2:2001 EMC - Part 4: Testing and measurement techniques - Section 4.2 Electrostatic discharge immunity test - Basic EMC Publication. (+/- 4KV contact and +/-8KV air discharge)

- IEC 61000-4-3:2003 EMC - Part 4. Testing and measurement techniques - Section 3: Radiated, radio-frequency, electromagnetic field immunity test

- IEC 61000-4-4:2004 EMC - Part 4: Testing and measurement techniques - Section 4: Electrical fast transient/burst immunity test - Basic EMC Publication

- IEC 61000-4-5:2001 EMC - Part 4: Testing and measurement techniques - Section 5: Surge immunity test

- IEC 61000-4-6:1996 EMC - Part 4: Testing and measurement techniques - Section 6: +A1:2001 Immunity to conducted disturbances induced by radio frequency fields

##

C.5 Regulatory Information

| Caution - If you make any modification to the AMC not expressly approved by Sun, you could void your warranty and/or regulatory authority to operate the component.

### C.5.1 FCC (USA)

This product has been tested and found to comply with the limits for a Class A digital device pursuant to Part 15 of the FCC rules. These limits are designed to provide reasonable protection against harmful interference when the equipment is operated in a commercial environment.

This product generates, uses, and can radiate radio frequency energy and, if not installed and used in accordance with the instruction manual, may cause harmful interference to radio communications. Operation of this equipment in a residential area is likely to cause harmful interference in which case the user will be required to correct the interference at the user’s own expense.

This AMC complies with Part 15 of the FCC Rules. Operation is subject to the following two conditions:

1. This device may not cause harmful interference.

2. This device must accept any interference received, including interference that may cause undesired operation.

### C.5.2 Industry Canada (Canada)

This Class A digital apparatus meets all requirements of the Canadian Interference Causing Equipment Regulations. Operation is subject to the following two conditions:

1. This device may not cause harmful interference.

2. This device must accept any interference received, including interference that may cause undesired operation.

Cet appareillage numérique de la classe A répond à toutes les exigences de l'interférence canadienne causant des règlements d'équipement. L'opération est sujette aux deux conditions suivantes:

1. Ce dispositif peut ne pas causer l'interférence nocive.

2. Ce dispositif doit accepter n'importe quelle interférence reçue, y compris l'interférence qui peut causer l'opération peu désirée.

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.