Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Fault Managment Command Examples

When no faults have been detected, the show fault output looks like this:

    -> show faulty
    Target              | Property               | Value
    --------------------+------------------------+-------------------

    -----------------------------------------------------------------

Other examples are shown in the following sections.

##### `show` `faulty` Example of a Power Supply Fault

The following is an example of the `show` `faulty` command reporting a power supply fault.

Note - The characters “SPT” at the beginning of the message ID indicate that the fault was detected by Oracle ILOM.

    -> show faulty
    Target              | Property               | Value
    --------------------+------------------------+-------------------------------
    /SP/faultmgmt/0     | fru                    | /SYS/PS0
    /SP/faultmgmt/0/    | class                  | fault.chassis.power.volt-fail
    faults/0            |                        |
    /SP/faultmgmt/0/    | sunw-msg-id            | SPT-8000-LC
    faults/0            |                        |
    /SP/faultmgmt/0/    | uuid                   | ********-****-****-****-************
    faults/0            |                        |
    /SP/faultmgmt/0/    | timestamp              | 2010-08-11/14:54:23
    faults/0            |                        |
    /SP/faultmgmt/0/    | fru_part_number        | *******
    faults/0            |                        |
    /SP/faultmgmt/0/    | fru_serial_number      | ******
    faults/0            |                        |
    /SP/faultmgmt/0/    | product_serial_number  | **********
    faults/0            |                        |
    /SP/faultmgmt/0/    | chassis_serial_number  | **********
    faults/0            |                        |
    /SP/faultmgmt/0/    | detector               | /SYS/PS0/VOLT_FAULT
    faults/0            |                        |

##### `fmadm` `faulty` Example of a Power Supply Fault

The following is an example of the `fmadm` `faulty` command reporting on the same power supply fault as shown in the `show` `faulty` example. Note that the two examples show the same UUID value.

The `fmadm` `faulty` command was invoked from within the Oracle ILOM `faultmgmt` shell.

Note - The characters “SPT” at the beginning of the message ID indicate that the fault was detected by Oracle ILOM.

    -> start /SP/faultmgmt/shell
    Are you sure you want to start /SP/faultmgmt/shell (y/n)? y

    faultmgmtsp> fmadm faulty
    ------------------- ------------------------------------ -------------- -------
    Time                UUID                                 msgid          Severity
    ------------------- ------------------------------------ -------------- -------
    2010-08-11/14:54:23 ********-****-****-****-************ SPT-8000-LC    Critical

    Fault class : fault.chassis.power.volt-fail

    Description : A Power Supply voltage level has exceeded acceptible limits.

    Response    : The service required LED on the chassis and on the affected
                  Power Supply may be illuminated.

    Impact      : Server will be powered down when there are insufficient
                  operational power supplies

    Action      : The administrator should review the ILOM event log for
                  additional information pertaining to this diagnosis.  Please
                  refer to the Details section of the Knowledge Article for
                  additional information.

    faultmgmtsp> exit

##### `show` `faulty` Example of a POST-Detected Fault

The following is an example of the `show` `faulty` command displaying a fault that was detected by POST. These kinds of faults are identified by the message `Forced` `fail` reason, where reason is the name of the power-on routine that detected the fault.

    -> show faulty
    Target             | Property               | Value
    -------------------+------------------------+--------------------------------
    /SP/faultmgmt/0    | fru                    | /SYS/MB
    /SP/faultmgmt/0    | class                  | fault.component.disabled
    faults/0           |                        |
    /SP/faultmgmt/0/   | sunw-msg-id            | SPT-8000-HR
    faults/0           |                        |
    /SP/faultmgmt/0/   | uuid                   | ********************************
    faults/0           |                        | a262
    /SP/faultmgmt/0/   | timestamp              | 2010-09-03/11:21:17
    faults/0           |                        |
    /SP/faultmgmt/0/   | detector               | /SYS/MB/CMP0/NIU1
    faults/0           |                        |
    /SP/faultmgmt/0/   | fru_part_number        | 541-3857-04
    faults/0           |                        |
    /SP/faultmgmt/0/   | fru_serial_number      | ******************
    faults/0           |                        |
    /SP/faultmgmt/0/   | product_serial_number  | **********
    faults/0           |                        |
    /SP/faultmgmt/0/   | chassis_serial_number  | **********
    faults/0           |                        |

##### `show` `faulty` Example of a PSH-Detected Fault

The following is an example of the `show` `faulty` command displaying a fault that was detected by the PSH technology. These kinds of faults are identified by the absence of the characters “SPT” at the beginning of the message ID.

    -> show faulty
    Target              | Property               | Value
    --------------------+------------------------+--------------------------------
    /SP/faultmgmt/0     | fru                    | /SYS/MB
    /SP/faultmgmt/0/    | class                  | fault.cpu.generic-sparc.strand
     faults/0           |                        |
    /SP/faultmgmt/0/    | sunw-msg-id            | SUN4V-8002-6E
    faults/0            |                        |
    /SP/faultmgmt/0/    | uuid                   | ********-****-****-****-************
    faults/0            |                        | 7a8a
    /SP/faultmgmt/0/    | timestamp              | 2010-08-13/15:48:33
    faults/0            |                        |
    /SP/faultmgmt/0/    | chassis_serial_number  | **********
    faults/0            |                        |
    /SP/faultmgmt/0/    | product_serial_number  | **********
    faults/0            |                        |
    /SP/faultmgmt/0/    | fru_serial_number      | *******-**********
    faults/0            |                        |
    /SP/faultmgmt/0/    | fru_part_number        | 541-3857-07
    faults/0            |                        |
    /SP/faultmgmt/0/    | mod-version            | 1.16
    faults/0            |                        |
    /SP/faultmgmt/0/    | mod-name               | eft
    faults/0            |                        |
    /SP/faultmgmt/0/    | fault_diagnosis        | /HOST
    faults/0            |                        |
    /SP/faultmgmt/0/    | severity               | Major
    faults/0            |                        |

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |