Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect a Terminal or Emulator to the SER MGT Port

Before You Begin

A null modem configuration is needed for DTE to DTE communications. You can use the supplied RJ-45 crossover adapter with a standard RJ-45 cable to achieve the null modem configuration.

1. Connect a terminal or a terminal emulator (PC or workstation) to the service processor serial management port.
2. Configure the terminal or terminal emulator with these settings:

   - 9600 baud

   - 8 bits

   - No parity

   - 1 Stop bit

   - No handshake

3. (Optional) Connect an Ethernet cable between the server's NET MGT port and the network to which future connections to the service processor and host will be made.

##### Related Information

- Oracle ILOM System Console Overview

- Power On the Server for the First Time

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |