Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### SP Network Address Options

You can access the SP on your system in multiple ways. Consider the following options and choose the access method that is best for your environment.

You can physically connect to the SP using a serial connection or a network connection. The network connection can be configured to use a static IP address or DHCP (the default). Optionally, the T3 Series servers can use an in-band network connection to the SP, rather than the default out-of-band network management port.

For more information on each option, see the following documentation:

- To use a serial connection to the SP, see:

  Connect a Terminal or Emulator to the SER MGT Port, in the installation guide for your server or Communicating With the Server Module During Startup in the installation guide for your server module.

- To assign a static IP address to the SP, see:

  Assign a Static IP Address to the SP, in the installation guide for your server.

- To use an in-band connection to the SP, see:

  Oracle ILOM In-band (Sideband) Management

##### Related Information

- Oracle Integrated Lights Out Manager (ILOM) 3.0 Documentation

- Oracle ILOM Overview

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |