Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the Ethernet Network Cables

Before You Begin

The server has four RJ-45 Gigabit Ethernet network connectors. They are marked NET0, NET1, NET2, and NET3.

1. Connect a Category 5 cable from your network switch or hub to Ethernet Port 0 (NET0) on the rear of the chassis.

   NET0 is the farthest left port in the 4-port network cluster.

   Figure 32 Service Processor Ethernet Network Ports – Rear Panel

2. Connect Category 5 cables from your network switch or hub to the remaining Ethernet ports (NET1, NET2, NET3), as needed.

##### Related Information

- Connecting the Server Cables

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |