Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Display the DHCP Server IP Address

To display the IP address of the DHCP server that provided the dynamic IP address requested by the service processor, view the `dhcp_server_ip` property.

- At the Oracle ILOM `->` prompt, type:

      -> show /SP/network

        /SP/network
           Targets:
               interconnect
               ipv6
               test

           Properties:
               commitpending = (Cannot show property)
               dhcp_server_ip = 10.8.31.5
               ipaddress = 10.8.31.188
               ipdiscovery = dhcp
               ipgateway = 10.8.31.248
               ipnetmask = 255.255.252.0
               macaddress = 00:14:4F:7E:83:4F
               managementport = /SYS/MB/SP/NETMGMT
               outofbandmacaddress = 00:21:28:8F:13:5F
               pendingipaddress = 10.8.31.188
               pendingipdiscovery = dhcp
               pendingipgateway = 10.8.31.248
               pendingipnetmask = 255.255.252.0
               sidebandmacaddress = 00:21:28:8F:13:5E
               state = enabled

           Commands:
               cd
               set
               show

  Note - The list of properties might vary based on your server.

##### Related Information

- Display the Host MAC Address

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |