Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a Hard Drive

Note - This is a hot service procedure that can be performed by customers while the server is running. See Hot Service, Replaceable by Customer for more information about hot service procedures.

1. With the latch open on the replacement drive, align insert the drive into the drive bay and slide it forward until it is seated.

   Tip - Drives are physically addressed according to the slot in which they are installed. If you are replacing a drive, install the replacement drive in the same slot as the drive that was removed.

2. Close the latch to lock the drive in place.
3. Bring the drive online.

   Configure the drive using the `cfgadm -c` `configure` command. In the following example, the drive at `c0::dsk/c1t1d0` will be configured.

       # cfgadm -c configure c0::dsk/c1t1d0

4. Verify the drive.

   See Verify the Functionality of a Hard Drive.

##### Related Information

- Remove a Hard Drive

- Verify the Functionality of a Hard Drive

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |