Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Create a Hardware RAID Volume

1. Prepare to create a RAID volume.

   See Prepare to Use the `FCode` Utility.

2. Use the `show-children` command to list the physical drives on the selected controller.

       {0} ok show-children

       FCode Version 1.00.54, MPT Version 2.00, Firmware Version 5.00.17.00

       Target 9
         Unit 0   Disk   SEAGATE  ST930003SSUN300G 0B70    585937500 Blocks, 300 GB
         SASDeviceName 5000c5001771776f  SASAddress 5000c5001771776d  PhyNum 0
       Target a
         Unit 0   Disk   SEAGATE  ST930003SSUN300G 0B70    585937500 Blocks, 300 GB
         SASDeviceName 5000c5001d0c38c7  SASAddress 5000c5001d0c38c5  PhyNum 1
       Target b
         Unit 0   Disk   SEAGATE  ST930003SSUN300G 0B70    585937500 Blocks, 300 GB
         SASDeviceName 5000c5001d097407  SASAddress 5000c5001d097405  PhyNum 2
       Target c
         Unit 0   Disk   SEAGATE  ST930003SSUN300G 0B70    585937500 Blocks, 300 GB
         SASDeviceName 5000c5001d09a51f  SASAddress 5000c5001d09a51d  PhyNum 3
       {0} ok

3. Use the `create-raid0-volume`, `create-raid1-volume`, or `create-raid1e-volume` command to create a logical drive from the physical disks.

   For example, to create a RAID 0 volume with targets 9 and a, type the targets first then type the `create` command:

       {0} ok 9 a create-raid0-volume

   For example, to create a RAID 1e volume with targets a, b, and c, type:

       {0} ok a b c create-raid1e-volume

4. To verify creation of the volume, type:

       {0} ok show-volumes

5. Type `unselect-dev` to deselect the controller.

       {0} ok unselect-dev

##### Related Information

- `FCode` Utility Commands

- Display the `ok` Prompt

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |