Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Configure Host Behavior With the Keyswitch State

Use the `/SYS keyswitch_state` property to control the position of the virtual keyswitch.

- At the Oracle ILOM `->` prompt, type:

      -> set /SYS keyswitch_state=value

  where value can be:

  - `normal` – The server can power itself on and start the boot process (the default).

  - `standby` – Powers off host, disables power on.

  - `diag` – Host power on is allowed, it overrides the settings of `/HOST/diag target`, resulting in Max POST being executed.

  - `locked` – Host power on is allowed, however, you are prohibited from updating any of the flash devices or setting `/HOST send_break_action=break`.

##### Related Information

- Power On the Server

- Power Off the Server

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |