Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Check for PSH-Detected Faults

The `fmadm` `faulty` command displays the list of faults detected by PSH. You can run this command either from the host or through the Oracle ILOM `fmadm` shell.

As an alternative, you can display fault information by running the Oracle ILOM command `show`.

1. Check the event log.

       # fmadm faulty
       TIME            EVENT-ID                              MSG-ID         SEVERITY
       Aug 13 11:48:33 f92e9fbe-735e-c218-cf87-9e1720a28004  SUN4V-8002-6E  Major

       Platform    : sun4v     Chassis_id  :
       Product_sn  :

       Fault class : fault.cpu.generic-sparc.strand
       Affects     : cpu:///cpuid=**/serial=*********************
                         faulted and taken out of service
       FRU         : "/SYS/MB"
       (hc://:product-id=*****:product-sn=**********:server-id=***-******-*****:
       chassis-id=********:**************-**********:serial=******:revision=05/
       chassis=0/motherboard=0)
                         faulty

       Description : The number of correctable errors associated with this strand has
                     exceeded acceptable levels.
                     Refer to http://sun.com/msg/SUN4V-8002-6E for more information.

       Response    : The fault manager will attempt to remove the affected strand
                     from service.

       Impact      : System performance may be affected.

       Action      : Schedule a repair procedure to replace the affected resource, the
                     identity of which can be determined using 'fmadm faulty'.

   In this example, a fault is displayed, indicating the following details:

   - Date and time of the fault (`Aug 13 11:48:33`).
   - EVENT-ID, which is unique for every fault (`21a8b59e-89ff-692a-c4bc-f4c5cccca8c8`).
   - MSG-ID, which can be used to obtain additional fault information (`SUN4V-8002-6E`).
   - Faulted FRU. The information provided in the example includes the part number of the FRU (`part=511127809`) and the serial number of the FRU (`serial=1005LCB-1019B100A2`). The FRU field provides the name of the FRU (/SYS/MB for motherboard in this example).
2. Use the MSG-ID to obtain more information about this type of fault:
   1. Obtain the MSG-ID from console output or from the Oracle ILOM `show` `faulty` command.
   2. Sign into the Oracle support site:

      http://support.oracle.com

   3. Type the MSG-ID in the Search Knowledge Base search window.

      The following example shows the knowledge article information provided for MSG-ID `SUN4V-8002-6E`.

          Correctable strand errors exceeded acceptable levels

          Type
              Fault
          Severity
              Major
          Description
               The number of correctable errors associated with this strand has exceeded
               acceptable levels.
          Automated Response
               The fault manager will attempt to remove the affected strand from service.
          Impact
               System performance may be affected.
          Suggested Action for System Administrator
               Schedule a repair procedure to replace the affected resource, the identity
               of which can be determined using fmadm faulty.
          Details
               There is no more information available at this time.

3. Follow the suggested actions to repair the fault.

##### Related Information

- PSH Overview

- PSH-Detected Fault Example (`show` `faulty` Command)

- Clear PSH-Detected Faults

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |