Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the Server From the Rack

The server must be removed from the rack to remove or install the following components:

- Motherboard

- Power distribution board

- Power supply backplane

- Connector card

- Hard drive backplane

- Front panel light-pipe assemblies

  | Caution - If necessary, use two people to dismount and carry the chassis.

1. Disconnect all the cables and power cords from the server.
2. Extend the server to the maintenance position.

   See Power Off the Server (SP Command).

3. Press the metal lever that is located on the inner side of the rail to disconnect the cable management arm (CMA) from the rail assembly, as shown in the following figure.

   The CMA is still attached to the cabinet, but the server chassis is now disconnected from the CMA.

   | Caution - If necessary, use two people to dismount and carry the chassis.

4. From the front of the server, pull the release tabs forward and pull the server forward until it is free of the rack rails as shown in the following figure.

   A release tab is located on each rail.

   Figure 48 Release Tabs and Slide Assembly

5. Set the server on a sturdy work surface.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |