Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Extend the Server

The following components can be serviced with the server in the maintenance position:

- Hard drives

- Fan modules

- DVD/USB module

- Fan power board

- PCIe/XAUI cards

- DDR3 DIMMs

- Motherboard battery

- SCC module

- Service processor module

If the server is installed in a rack with extendable slide rails, use this procedure to extend the server to the maintenance position.

1. (Optional) Use the `set /SYS/LOCATE` command from the `->` prompt to locate the system that requires maintenance.

       -> set /SYS/LOCATE value=Fast_Blink

   Once you have located the server, press the Locator LED and button to turn it off.

2. Verify that no cables will be damaged or will interfere when the server is extended.

   Although the CMA that is supplied with the server is hinged to accommodate extending the server, you should ensure that all cables and cords are capable of extending.

3. From the front of the server, release the two slide release latches, as shown in the following figure.

   Squeeze the green slide release latches to release the slide rails.

   Figure 47 Slide Release Latches

4. While squeezing the slide release latches, slowly pull the server forward until the slide rails latch.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |