Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a PCIe or PCIe/XAUI Riser

Note - This is a cold service procedure that can be performed by customers. See Cold Service, Replaceable by Customer for more information about cold service procedures.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

| Caution - Components inside the chassis might be hot. Use caution when servicing components inside the chassis.

1. Perform the preliminary steps required for cold service procedures.

   See Cold Service, Replaceable by Customer for instructions.

2. Extend the server to the maintenance position.

   See Extend the Server.

3. Remove the top cover.

   See Remove the Top Cover.

4. Attach an antistatic wrist strap.
5. Align the riser board with the riser connector and press down to engage the connector (panel 1).
6. Tighten the riser screw (panel 2).
7. Slide the crossbeam into position between the power supply bay and the side of the chassis (panel 3).
8. Tighten the two captive screws to secure the crossbeam (panel 4)

##### Related Information

- Remove a PCIe or PCIe/XAUI Riser

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |