Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a DIMM

Note - This is a cold service procedure that can be performed by customers. See Cold Service, Replaceable by Customer for more information about cold service procedures.

1. Perform the preliminary steps required for cold service procedures.

   See Cold Service, Replaceable by Customer for instructions.

2. Extend the server to the maintenance position.

   See Extend the Server

3. Attach an antistatic wrist strap.
4. Remove the top cover.

   See Remove the Top Cover

5. Swing the air duct up and forward to the fully open position.
6. Unpack the replacement DIMMs and place them on an antistatic mat.
7. Ensure that the ejector tabs on the connector that will receive the DIMM are in the open position.

   Figure 49 Installing DIMMs

8. Align the DIMM notch with the key in the connector.

   | Caution - Ensure that the orientation is correct. The DIMM might be damaged if the orientation is reversed.

9. Push the DIMM into the connector until the ejector tabs lock the DIMM in place.

   If the DIMM does not easily seat into the connector, check the DIMM's orientation.

10. Repeat Step 7 through Step 9 until all new DIMMs are installed.
11. Return the air duct to the closed position.
12. Install the top cover.

    See Install the Top Cover.

13. Slide the server into the rack.

    See Reinstall the Server in the Rack.

14. Connect the power cords.

    See.Reconnect the Power Cords.

    Note - As soon as the power cords are connected, standby power is applied. Depending on how the firmware is configured, the system might boot at this time.

    | Caution - Do not leave DIMM slots empty. You must install filler panels in all empty DIMM slots.

##### Related Information

- Remove a DIMM

- Increase System Memory With Additional DIMMs

- Verify DIMM Functionality

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |