Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Prepare the Power Cords

The service processor runs on the 3.3V standby voltage, which becomes available as soon as a power source is connected to the server. If you do not want the server to start the initialization diagnostics at this point, connect only the power supply end of the power cord(s).

- Plug the power cords into the power supplies.

  Note - Do not connect the power cords to the power sources at this time. Doing so will cause you to miss system initialization and diagnostic messages that are output during the power-up phase.

##### Related Information

- Connect a Terminal or Emulator to the SER MGT Port

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |