Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Top Cover

1. Place the top cover on the chassis.

   Set the cover down so that it hangs over the rear of the server by about an inch (25.4 mm).

2. Slide the top cover forward until it seats.

   Note - If an emergency shutdown occurred when the top cover was removed, you must install the top cover and use the `poweron` command to restart the system. See Power On the Server (`start /SYS` Command) for more information about the `poweron` command.

##### Related Information

- Power On the Server (`start /SYS` Command)

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |